<?xml version="1.0" encoding="UTF-8"?>
<EnsembleReport name="NIOS_LED" kind="system" version="16.0" fabric="QSYS">
 <!-- Format version 16.0 211 (Future versions may contain additional information.) -->
 <!-- 2017.06.27.19:35:24 -->
 <!-- A collection of modules and connections -->
 <parameter name="clockCrossingAdapter">
  <type>com.altera.sopcmodel.ensemble.EClockAdapter</type>
  <value>HANDSHAKE</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="device">
  <type>java.lang.String</type>
  <value>10M08DAF256C8GES</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="deviceFamily">
  <type>java.lang.String</type>
  <value>MAX10FPGA</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="deviceSpeedGrade">
  <type>java.lang.String</type>
  <value>8</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="fabricMode">
  <type>com.altera.sopcmodel.ensemble.Ensemble$EFabricMode</type>
  <value>QSYS</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="generateLegacySim">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="generationId">
  <type>int</type>
  <value>1498584906</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="globalResetBus">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="hdlLanguage">
  <type>com.altera.entityinterfaces.moduleext.IModuleGenerateHDL$HDLLanguage</type>
  <value>VERILOG</value>
  <derived>false</derived>
  <enabled>false</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="hideFromIPCatalog">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="lockedInterfaceDefinition">
  <type>com.altera.sopcmodel.definition.BoundaryDefinition</type>
  <value></value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="maxAdditionalLatency">
  <type>int</type>
  <value>1</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>true</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="projectName">
  <type>java.lang.String</type>
  <value>NIOS_LED.qpf</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="sopcBorderPoints">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="systemHash">
  <type>long</type>
  <value>0</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="testBenchDutName">
  <type>java.lang.String</type>
  <value></value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="timeStamp">
  <type>long</type>
  <value>0</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <parameter name="useTestBenchNamingPattern">
  <type>boolean</type>
  <value>false</value>
  <derived>false</derived>
  <enabled>true</enabled>
  <visible>false</visible>
  <valid>true</valid>
 </parameter>
 <module name="clk_0" kind="clock_source" version="16.0" path="clk_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="clockFrequency">
   <type>long</type>
   <value>20000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="clockFrequencyKnown">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="inputClockFrequency">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk_in</sysinfo_arg>
  </parameter>
  <parameter name="resetSynchronousEdges">
   <type>com.altera.sopcmodel.reset.Reset$Edges</type>
   <value>NONE</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk_in" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>qsys.ui.export_name</name>
    <value>clk</value>
   </assignment>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>20000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>in_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="clk_in_reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>qsys.ui.export_name</name>
    <value>reset</value>
   </assignment>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="clk" kind="clock_source" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedDirectClock">
    <type>java.lang.String</type>
    <value>clk_in</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>long</type>
    <value>20000000</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>true</isStart>
   <port>
    <name>clk_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clk</role>
   </port>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>nios2_gen2_0</moduleName>
    <slaveName>clk</slaveName>
    <name>nios2_gen2_0.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>timer_0</moduleName>
    <slaveName>clk</slaveName>
    <name>timer_0.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>pio_0</moduleName>
    <slaveName>clk</slaveName>
    <name>pio_0.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>clk1</slaveName>
    <name>onchip_memory2_0.clk1</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>hex7led_0</moduleName>
    <slaveName>clock</slaveName>
    <name>hex7led_0.clock</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_0</moduleName>
    <slaveName>clk_0_clk</slaveName>
    <name>mm_interconnect_0.clk_0_clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>irq_mapper</moduleName>
    <slaveName>clk</slaveName>
    <name>irq_mapper.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>rst_controller</moduleName>
    <slaveName>clk</slaveName>
    <name>rst_controller.clk</name>
   </clockDomainMember>
   <clockDomainMember>
    <isBridge>false</isBridge>
    <moduleName>rst_translator</moduleName>
    <slaveName>clk</slaveName>
    <name>rst_translator.clk</name>
   </clockDomainMember>
  </interface>
  <interface name="clk_reset" kind="reset_source" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value>clk_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>clk_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_n_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
 </module>
 <module name="hex7led_0" kind="hex7led" version="1.0" path="hex7led_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="avalon_slave_0" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>2</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clock</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>x</name>
    <direction>Input</direction>
    <width>16</width>
    <role>writedata</role>
   </port>
   <port>
    <name>write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>chipselect</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>byteenable</name>
    <direction>Input</direction>
    <width>2</width>
    <role>byteenable</role>
   </port>
  </interface>
  <interface name="clock" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clock</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>resetn</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="segment" kind="conduit_end" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clock</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>seg</name>
    <direction>Output</direction>
    <width>8</width>
    <role>new_signal</role>
   </port>
  </interface>
  <interface name="digit" kind="conduit_end" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clock</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>dig</name>
    <direction>Output</direction>
    <width>4</width>
    <role>new_signal</role>
   </port>
  </interface>
 </module>
 <module
   name="nios2_gen2_0"
   kind="altera_nios2_gen2"
   version="16.0"
   path="nios2_gen2_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>debug.hostConnection</name>
   <value>type jtag id 70:34|110:135</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.BIG_ENDIAN</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.BREAK_ADDR</name>
   <value>0x00010820</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CPU_ARCH_NIOS2_R1</name>
   <value></value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CPU_FREQ</name>
   <value>20000000u</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CPU_ID_SIZE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CPU_ID_VALUE</name>
   <value>0x00000000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CPU_IMPLEMENTATION</name>
   <value>"tiny"</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DATA_ADDR_WIDTH</name>
   <value>17</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DCACHE_LINE_SIZE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DCACHE_LINE_SIZE_LOG2</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DCACHE_SIZE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.EXCEPTION_ADDR</name>
   <value>0x00008020</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FLASH_ACCELERATOR_LINES</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FLASH_ACCELERATOR_LINE_SIZE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FLUSHDA_SUPPORTED</name>
   <value></value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HARDWARE_DIVIDE_PRESENT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HARDWARE_MULTIPLY_PRESENT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HARDWARE_MULX_PRESENT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_DEBUG_CORE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_DEBUG_STUB</name>
   <value></value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_ILLEGAL_INSTRUCTION_EXCEPTION</name>
   <value></value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_JMPI_INSTRUCTION</name>
   <value></value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.ICACHE_LINE_SIZE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.ICACHE_LINE_SIZE_LOG2</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.ICACHE_SIZE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INST_ADDR_WIDTH</name>
   <value>17</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.OCI_VERSION</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.RESET_ADDR</name>
   <value>0x00008000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.DataCacheVictimBufImpl</name>
   <value>ram</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.HDLSimCachesCleared</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.breakOffset</name>
   <value>32</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.breakSlave</name>
   <value>nios2_gen2_0.debug_mem_slave</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.cpuArchitecture</name>
   <value>Nios II</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.exceptionOffset</name>
   <value>32</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.exceptionSlave</name>
   <value>onchip_memory2_0.s1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.resetOffset</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.configuration.resetSlave</name>
   <value>onchip_memory2_0.s1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.compatible</name>
   <value>altr,nios2-1.1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.group</name>
   <value>cpu</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.name</name>
   <value>nios2</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.altr,exception-addr</name>
   <value>0x00008020</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.altr,implementation</name>
   <value>"tiny"</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.altr,reset-addr</name>
   <value>0x00008000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.clock-frequency</name>
   <value>20000000u</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.dcache-line-size</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.dcache-size</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.icache-line-size</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.icache-size</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.vendor</name>
   <value>altr</value>
  </assignment>
  <parameter name="tmr_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_disable_tmr_inj">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_showUnpublishedSettings">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_showInternalSettings">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_preciseIllegalMemAccessException">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_exportPCB">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_exportdebuginfo">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_clearXBitsLDNonBypass">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_bigEndian">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_export_large_RAMs">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_asic_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_asic_synopsys_translate_on_off">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_asic_third_party_synthesis">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_asic_add_scan_mode_input">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_oci_version">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_fast_register_read">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_exportHostDebugPort">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_oci_export_jtag_signals">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_avalonDebugPortPresent">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_alwaysEncrypt">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="io_regionbase">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="io_regionsize">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_support31bitdcachebypass">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_activateTrace">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_allow_break_inst">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_activateTestEndChecker">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_ecc_sim_test_ports">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_disableocitrace">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_activateMonitors">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_HDLSimCachesCleared">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_HBreakTest">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_breakslaveoveride">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_useLimit">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_autoAssignTlbPtrSz">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cpuReset">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetrequest_enabled">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_removeRAMinit">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_tmr_output_disable">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_shadowRegisterSets">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_numOfInstRegion">
   <type>int</type>
   <value>8</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_numOfDataRegion">
   <type>int</type>
   <value>8</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_TLBMissExcOffset">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetOffset">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="exceptionOffset">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cpuID">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="breakOffset">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="userDefinedSettings">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tracefilename">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetSlave">
   <type>java.lang.String</type>
   <value>onchip_memory2_0.s1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_TLBMissExcSlave">
   <type>java.lang.String</type>
   <value>None</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="exceptionSlave">
   <type>java.lang.String</type>
   <value>onchip_memory2_0.s1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="breakSlave">
   <type>java.lang.String</type>
   <value>None</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_interruptControllerType">
   <type>java.lang.String</type>
   <value>Internal</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_branchpredictiontype">
   <type>java.lang.String</type>
   <value>Dynamic</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_bhtPtrSz">
   <type>int</type>
   <value>8</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cpuArchRev">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="stratix_dspblock_shift_mul">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="shifterType">
   <type>java.lang.String</type>
   <value>medium_le_shift</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="multiplierType">
   <type>java.lang.String</type>
   <value>no_mul</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mul_shift_choice">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mul_32_impl">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mul_64_impl">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="shift_rot_impl">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dividerType">
   <type>java.lang.String</type>
   <value>no_div</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_minInstRegionSize">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpu_minDataRegionSize">
   <type>int</type>
   <value>12</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_uitlbNumEntries">
   <type>int</type>
   <value>4</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_udtlbNumEntries">
   <type>int</type>
   <value>6</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_tlbPtrSz">
   <type>int</type>
   <value>7</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_tlbNumWays">
   <type>int</type>
   <value>16</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_processIDNumBits">
   <type>int</type>
   <value>8</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="impl">
   <type>java.lang.String</type>
   <value>Tiny</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="icache_size">
   <type>int</type>
   <value>4096</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fa_cache_line">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fa_cache_linesize">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="icache_tagramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="icache_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="icache_numTCIM">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="icache_burstType">
   <type>java.lang.String</type>
   <value>None</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_bursts">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_victim_buf_impl">
   <type>java.lang.String</type>
   <value>ram</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_size">
   <type>int</type>
   <value>2048</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_tagramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_numTCDM">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_exportvectors">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_usedesignware">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_ecc_present">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_ic_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_rf_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_mmu_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_dc_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_itcm_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_dtcm_ecc_present">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="regfile_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ocimem_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ocimem_ramInit">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bht_ramBlockType">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="cdx_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mpx_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_enabled">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_triggerArming">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_debugReqSignals">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_assignJtagInstanceID">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_jtagInstanceID">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_OCIOnchipTrace">
   <type>java.lang.String</type>
   <value>_128</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_hwbreakpoint">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_datatrigger">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_traceType">
   <type>java.lang.String</type>
   <value>none</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_traceStorage">
   <type>java.lang.String</type>
   <value>onchip_trace</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="master_addr_map">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instruction_master_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instruction_master_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flash_instruction_master_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="flash_instruction_master_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="data_master_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="data_master_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_0_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_0_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_1_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_1_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_2_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_2_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_3_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_instruction_master_3_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_0_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_0_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_1_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_1_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_2_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_2_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_3_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="tightly_coupled_data_master_3_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instruction_master_high_performance_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instruction_master_high_performance_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="data_master_high_performance_paddr_base">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="data_master_high_performance_paddr_size">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetAbsoluteAddr">
   <type>int</type>
   <value>32768</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="exceptionAbsoluteAddr">
   <type>int</type>
   <value>32800</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="breakAbsoluteAddr">
   <type>int</type>
   <value>67616</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mmu_TLBMissExcAbsAddr">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_bursts_derived">
   <type>java.lang.String</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_size_derived">
   <type>int</type>
   <value>2048</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="breakSlave_derived">
   <type>java.lang.String</type>
   <value>nios2_gen2_0.debug_mem_slave</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dcache_lineSize_derived">
   <type>int</type>
   <value>32</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_ioregionBypassDCache">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="setting_bit31BypassDCache">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="translate_on">
   <type>java.lang.String</type>
   <value> "synthesis translate_on"  </value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="translate_off">
   <type>java.lang.String</type>
   <value> "synthesis translate_off" </value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_onchiptrace">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_offchiptrace">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_insttrace">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="debug_datatrace">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instAddrWidth">
   <type>int</type>
   <value>17</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>instruction_master</sysinfo_arg>
  </parameter>
  <parameter name="faAddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>flash_instruction_master</sysinfo_arg>
  </parameter>
  <parameter name="dataAddrWidth">
   <type>int</type>
   <value>17</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>data_master</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster0AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_0</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster1AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_1</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster2AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_2</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster3AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_3</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster0AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_0</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster1AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_1</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster2AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_2</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster3AddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_3</sysinfo_arg>
  </parameter>
  <parameter name="dataMasterHighPerformanceAddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>data_master_high_performance</sysinfo_arg>
  </parameter>
  <parameter name="instructionMasterHighPerformanceAddrWidth">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_WIDTH</sysinfo_type>
   <sysinfo_arg>instruction_master_high_performance</sysinfo_arg>
  </parameter>
  <parameter name="instSlaveMapParam">
   <type>java.lang.String</type>
   <value><![CDATA[<address-map><slave name='onchip_memory2_0.s1' start='0x8000' end='0x10000' type='altera_avalon_onchip_memory2.s1' /><slave name='nios2_gen2_0.debug_mem_slave' start='0x10800' end='0x11000' type='altera_nios2_gen2.debug_mem_slave' /></address-map>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>instruction_master</sysinfo_arg>
  </parameter>
  <parameter name="faSlaveMapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>flash_instruction_master</sysinfo_arg>
  </parameter>
  <parameter name="dataSlaveMapParam">
   <type>java.lang.String</type>
   <value><![CDATA[<address-map><slave name='onchip_memory2_0.s1' start='0x8000' end='0x10000' type='altera_avalon_onchip_memory2.s1' /><slave name='nios2_gen2_0.debug_mem_slave' start='0x10800' end='0x11000' type='altera_nios2_gen2.debug_mem_slave' /><slave name='timer_0.s1' start='0x11000' end='0x11020' type='altera_avalon_timer.s1' /><slave name='pio_0.s1' start='0x11020' end='0x11030' type='altera_avalon_pio.s1' /><slave name='hex7led_0.avalon_slave_0' start='0x11030' end='0x11032' type='hex7led.avalon_slave_0' /></address-map>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>data_master</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster0MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_0</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster1MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_1</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster2MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_2</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledDataMaster3MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_data_master_3</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster0MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_0</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster1MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_1</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster2MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_2</sysinfo_arg>
  </parameter>
  <parameter name="tightlyCoupledInstructionMaster3MapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>tightly_coupled_instruction_master_3</sysinfo_arg>
  </parameter>
  <parameter name="dataMasterHighPerformanceMapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>data_master_high_performance</sysinfo_arg>
  </parameter>
  <parameter name="instructionMasterHighPerformanceMapParam">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>ADDRESS_MAP</sysinfo_type>
   <sysinfo_arg>instruction_master_high_performance</sysinfo_arg>
  </parameter>
  <parameter name="clockFrequency">
   <type>long</type>
   <value>20000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamilyName">
   <type>java.lang.String</type>
   <value>MAX10FPGA</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="internalIrqMaskSystemInfo">
   <type>long</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>INTERRUPTS_USED</sysinfo_type>
   <sysinfo_arg>irq</sysinfo_arg>
  </parameter>
  <parameter name="customInstSlavesSystemInfo">
   <type>java.lang.String</type>
   <value><![CDATA[<info/>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CUSTOM_INSTRUCTION_SLAVES</sysinfo_type>
   <sysinfo_arg>custom_instruction_master</sysinfo_arg>
  </parameter>
  <parameter name="customInstSlavesSystemInfo_nios_a">
   <type>java.lang.String</type>
   <value><![CDATA[<info/>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CUSTOM_INSTRUCTION_SLAVES</sysinfo_type>
   <sysinfo_arg>custom_instruction_master_a</sysinfo_arg>
  </parameter>
  <parameter name="customInstSlavesSystemInfo_nios_b">
   <type>java.lang.String</type>
   <value><![CDATA[<info/>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CUSTOM_INSTRUCTION_SLAVES</sysinfo_type>
   <sysinfo_arg>custom_instruction_master_b</sysinfo_arg>
  </parameter>
  <parameter name="customInstSlavesSystemInfo_nios_c">
   <type>java.lang.String</type>
   <value><![CDATA[<info/>]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CUSTOM_INSTRUCTION_SLAVES</sysinfo_type>
   <sysinfo_arg>custom_instruction_master_c</sysinfo_arg>
  </parameter>
  <parameter name="deviceFeaturesSystemInfo">
   <type>java.lang.String</type>
   <value>ADDRESS_STALL 1 ADVANCED_INFO 0 ALLOWS_COMPILING_OTHER_FAMILY_IP 1 ANY_QFP 0 CELL_LEVEL_BACK_ANNOTATION_DISABLED 0 COMPILER_SUPPORT 1 DSP 1 DSP_SHIFTER_BLOCK 0 DUMP_ASM_LAB_BITS_FOR_POWER 1 EMUL 0 ENABLE_ADVANCED_IO_ANALYSIS_GUI_FEATURES 0 ENABLE_PHYSICAL_DESIGN_PLANNER 0 ENABLE_PIN_PLANNER 0 ENGINEERING_SAMPLE 0 EPCS 1 ESB 0 FAKE1 0 FAKE2 0 FAKE3 0 FAMILY_LEVEL_INSTALLATION_ONLY 0 FASTEST 0 FINAL_TIMING_MODEL 0 FITTER_USE_FALLING_EDGE_DELAY 1 FPP_COMPLETELY_PLACES_AND_ROUTES_PERIPHERY 0 GENERATE_DC_ON_CURRENT_WARNING_FOR_INTERNAL_CLAMPING_DIODE 0 HARDCOPY 0 HAS_18_BIT_MULTS 0 HAS_ACE_SUPPORT 1 HAS_ACTIVE_PARALLEL_FLASH_SUPPORT 0 HAS_ADJUSTABLE_OUTPUT_IO_TIMING_MEAS_POINT 1 HAS_ADVANCED_IO_INVERTED_CORNER 0 HAS_ADVANCED_IO_POWER_SUPPORT 1 HAS_ADVANCED_IO_TIMING_SUPPORT 1 HAS_ALM_SUPPORT 0 HAS_ATOM_AND_ROUTING_POWER_MODELED_TOGETHER 0 HAS_AUTO_DERIVE_CLOCK_UNCERTAINTY_SUPPORT 0 HAS_AUTO_FIT_SUPPORT 1 HAS_BALANCED_OPT_TECHNIQUE_SUPPORT 1 HAS_BENEFICIAL_SKEW_SUPPORT 1 HAS_BITLEVEL_DRIVE_STRENGTH_CONTROL 0 HAS_BSDL_FILE_GENERATION 0 HAS_CDB_RE_NETWORK_PRESERVATION_SUPPORT 0 HAS_CGA_SUPPORT 1 HAS_CHECK_NETLIST_SUPPORT 0 HAS_CLOCK_REGION_CHECKER_ENABLED 1 HAS_CORE_JUNCTION_TEMP_DERATING 0 HAS_CROSSTALK_SUPPORT 0 HAS_CUSTOM_REGION_SUPPORT 1 HAS_DAP_JTAG_FROM_HPS 0 HAS_DATA_DRIVEN_ACVQ_HSSI_SUPPORT 0 HAS_DDB_FDI_SUPPORT 0 HAS_DESIGN_ANALYZER_SUPPORT 0 HAS_DETAILED_IO_RAIL_POWER_MODEL 1 HAS_DETAILED_LEIM_STATIC_POWER_MODEL 0 HAS_DETAILED_LE_POWER_MODEL 1 HAS_DETAILED_ROUTING_MUX_STATIC_POWER_MODEL 0 HAS_DETAILED_THERMAL_CIRCUIT_PARAMETER_SUPPORT 1 HAS_DEVICE_MIGRATION_SUPPORT 1 HAS_DIAGONAL_MIGRATION_SUPPORT 0 HAS_EMIF_TOOLKIT_SUPPORT 0 HAS_ERROR_DETECTION_SUPPORT 0 HAS_FAMILY_VARIANT_MIGRATION_SUPPORT 0 HAS_FANOUT_FREE_NODE_SUPPORT 1 HAS_FAST_FIT_SUPPORT 1 HAS_FITTER_ECO_SUPPORT 1 HAS_FIT_NETLIST_OPT_RETIME_SUPPORT 1 HAS_FIT_NETLIST_OPT_SUPPORT 1 HAS_FORMAL_VERIFICATION_SUPPORT 0 HAS_FPGA_XCHANGE_SUPPORT 0 HAS_FSAC_LUTRAM_REGISTER_PACKING_SUPPORT 0 HAS_FULL_DAT_MIN_TIMING_SUPPORT 1 HAS_FULL_INCREMENTAL_DESIGN_SUPPORT 1 HAS_FUNCTIONAL_SIMULATION_SUPPORT 1 HAS_FUNCTIONAL_VERILOG_SIMULATION_SUPPORT 0 HAS_FUNCTIONAL_VHDL_SIMULATION_SUPPORT 0 HAS_GLITCH_FILTERING_SUPPORT 1 HAS_HARDCOPYII_SUPPORT 0 HAS_HC_READY_SUPPORT 0 HAS_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_HOLD_TIME_AVOIDANCE_ACROSS_CLOCK_SPINE_SUPPORT 1 HAS_HSPICE_WRITER_SUPPORT 0 HAS_HSSI_POWER_CALCULATOR 1 HAS_IBISO_WRITER_SUPPORT 0 HAS_ICD_DATA_IP 0 HAS_IDB_SUPPORT 0 HAS_INCREMENTAL_DAT_SUPPORT 1 HAS_INCREMENTAL_SYNTHESIS_SUPPORT 1 HAS_IO_ASSIGNMENT_ANALYSIS_SUPPORT 1 HAS_IO_DECODER 0 HAS_IO_PLACEMENT_OPTIMIZATION_SUPPORT 1 HAS_IO_PLACEMENT_USING_GEOMETRY_RULE 0 HAS_IO_PLACEMENT_USING_PHYSIC_RULE 0 HAS_IO_SMART_RECOMPILE_SUPPORT 0 HAS_JITTER_SUPPORT 1 HAS_JTAG_SLD_HUB_SUPPORT 1 HAS_LOGIC_LOCK_SUPPORT 1 HAS_MICROPROCESSOR 0 HAS_MIF_SMART_COMPILE_SUPPORT 1 HAS_MINMAX_TIMING_MODELING_SUPPORT 1 HAS_MIN_TIMING_ANALYSIS_SUPPORT 1 HAS_MUX_RESTRUCTURE_SUPPORT 1 HAS_NADDER_STYLE_CLOCKING 0 HAS_NADDER_STYLE_FF 0 HAS_NADDER_STYLE_LCELL_COMB 0 HAS_NEW_CDB_NAME_FOR_M20K_SCLR 0 HAS_NEW_HC_FLOW_SUPPORT 0 HAS_NEW_SERDES_MAX_RESOURCE_COUNT_REPORTING_SUPPORT 1 HAS_NEW_VPR_SUPPORT 1 HAS_NONSOCKET_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_NO_HARDBLOCK_PARTITION_SUPPORT 0 HAS_NO_JTAG_USERCODE_SUPPORT 0 HAS_OPERATING_SETTINGS_AND_CONDITIONS_REPORTING_SUPPORT 1 HAS_PAD_LOCATION_ASSIGNMENT_SUPPORT 0 HAS_PARTIAL_RECONFIG_SUPPORT 0 HAS_PASSIVE_PARALLEL_SUPPORT 0 HAS_PHYSICAL_DESIGN_PLANNER_SUPPORT 0 HAS_PHYSICAL_NETLIST_OUTPUT 0 HAS_PHYSICAL_ROUTING_SUPPORT 0 HAS_PIN_SPECIFIC_VOLTAGE_SUPPORT 1 HAS_PLDM_REF_SUPPORT 0 HAS_POWER_BINNING_LIMITS_DATA 1 HAS_POWER_ESTIMATION_SUPPORT 1 HAS_PRELIMINARY_CLOCK_UNCERTAINTY_NUMBERS 0 HAS_PRE_FITTER_FPP_SUPPORT 0 HAS_PRE_FITTER_LUTRAM_NETLIST_CHECKER_ENABLED 0 HAS_PVA_SUPPORT 1 HAS_QUARTUS_HIERARCHICAL_DESIGN_SUPPORT 0 HAS_RAPID_RECOMPILE_SUPPORT 0 HAS_RCF_SUPPORT 1 HAS_RCF_SUPPORT_FOR_DEBUGGING 0 HAS_RED_BLACK_SEPARATION_SUPPORT 0 HAS_RE_LEVEL_TIMING_GRAPH_SUPPORT 1 HAS_RISEFALL_DELAY_SUPPORT 1 HAS_SIGNAL_PROBE_SUPPORT 1 HAS_SIGNAL_TAP_SUPPORT 1 HAS_SIMULATOR_SUPPORT 0 HAS_SPLIT_IO_SUPPORT 1 HAS_SPLIT_LC_SUPPORT 1 HAS_STRICT_PRESERVATION_SUPPORT 1 HAS_SYNTHESIS_ON_ATOMS 0 HAS_SYNTH_FSYN_NETLIST_OPT_SUPPORT 1 HAS_SYNTH_NETLIST_OPT_RETIME_SUPPORT 0 HAS_SYNTH_NETLIST_OPT_SUPPORT 1 HAS_TCL_FITTER_SUPPORT 0 HAS_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_TEMPLATED_REGISTER_PACKING_SUPPORT 1 HAS_TIME_BORROWING_SUPPORT 0 HAS_TIMING_DRIVEN_SYNTHESIS_SUPPORT 1 HAS_TIMING_INFO_SUPPORT 1 HAS_TIMING_OPERATING_CONDITIONS 1 HAS_TIMING_SIMULATION_SUPPORT 0 HAS_TITAN_BASED_MAC_REGISTER_PACKER_SUPPORT 0 HAS_U2B2_SUPPORT 0 HAS_USER_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_USE_FITTER_INFO_SUPPORT 1 HAS_VCCPD_POWER_RAIL 0 HAS_VERTICAL_MIGRATION_SUPPORT 1 HAS_VIEWDRAW_SYMBOL_SUPPORT 0 HAS_VIO_SUPPORT 1 HAS_VIRTUAL_DEVICES 0 HAS_WYSIWYG_DFFEAS_SUPPORT 1 HAS_XIBISO2_WRITER_SUPPORT 1 HAS_XIBISO_WRITER_SUPPORT 0 IFP_USE_LEGACY_IO_CHECKER 0 INCREMENTAL_DESIGN_SUPPORTS_COMPATIBLE_CONSTRAINTS 1 INSTALLED 0 INTERNAL_POF_SUPPORT_ENABLED 0 INTERNAL_USE_ONLY 0 ISSUE_MILITARY_TEMPERATURE_WARNING 0 IS_CONFIG_ROM 0 IS_DEFAULT_FAMILY 0 IS_FOR_INTERNAL_TESTING_ONLY 0 IS_HARDCOPY_FAMILY 0 IS_HBGA_PACKAGE 0 IS_HIGH_CURRENT_PART 0 IS_LOW_POWER_PART 0 IS_SDM_ONLY_PACKAGE 0 IS_SMI_PART 0 LOAD_BLK_TYPE_DATA_FROM_ATOM_WYS_INFO 0 LVDS_IO 0 M10K_MEMORY 0 M144K_MEMORY 0 M20K_MEMORY 0 M4K_MEMORY 0 M512_MEMORY 0 M9K_MEMORY 1 MLAB_MEMORY 0 MRAM_MEMORY 0 NOT_LISTED 0 NOT_MIGRATABLE 0 NO_FITTER_DELAY_CACHE_GENERATED 0 NO_PIN_OUT 0 NO_POF 0 NO_RPE_SUPPORT 0 NO_SUPPORT_FOR_LOGICLOCK_CONTENT_BACK_ANNOTATION 0 NO_SUPPORT_FOR_STA_CLOCK_UNCERTAINTY_CHECK 0 NO_TDC_SUPPORT 0 POSTFIT_BAK_DATABASE_EXPORT_ENABLED 0 POSTMAP_BAK_DATABASE_EXPORT_ENABLED 0 PROGRAMMER_ONLY 0 PROGRAMMER_SUPPORT 1 PVA_SUPPORTS_ONLY_SUBSET_OF_ATOMS 0 QFIT_IN_DEVELOPMENT 0 QMAP_IN_DEVELOPMENT 0 RAM_LOGICAL_NAME_CHECKING_IN_CUT_ENABLED 1 REPORTS_METASTABILITY_MTBF 1 REQUIRES_INSTALLATION_PATCH 0 REQUIRES_LIST_OF_TEMPERATURE_AND_VOLTAGE_OPERATING_CONDITIONS 1 REQUIRE_QUARTUS_HIERARCHICAL_DESIGN 0 REQUIRE_SPECIAL_HANDLING_FOR_LOCAL_LABLINE 1 RESERVES_SIGNAL_PROBE_PINS 0 RESOLVE_MAX_FANOUT_EARLY 1 RESOLVE_MAX_FANOUT_LATE 0 RESPECTS_FIXED_SIZED_LOCKED_LOCATION_LOGICLOCK 1 RESTRICTED_USER_SELECTION 0 RESTRICT_PARTIAL_RECONFIG 0 RISEFALL_SUPPORT_IS_HIDDEN 0 SHOW_HIDDEN_FAMILY_IN_PROGRAMMER 0 STRICT_TIMING_DB_CHECKS 0 SUPPORTS_ADDITIONAL_OPTIONS_FOR_UNUSED_IO 0 SUPPORTS_CRC 1 SUPPORTS_DIFFERENTIAL_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_DSP_BALANCING_BACK_ANNOTATION 0 SUPPORTS_GENERATION_OF_EARLY_POWER_ESTIMATOR_FILE 1 SUPPORTS_GLOBAL_SIGNAL_BACK_ANNOTATION 0 SUPPORTS_HIPI_RETIMING 0 SUPPORTS_MAC_CHAIN_OUT_ADDER 0 SUPPORTS_RAM_PACKING_BACK_ANNOTATION 0 SUPPORTS_REG_PACKING_BACK_ANNOTATION 0 SUPPORTS_SIGNALPROBE_REGISTER_PIPELINING 1 SUPPORTS_SINGLE_ENDED_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_USER_MANUAL_LOGIC_DUPLICATION 1 SUPPORTS_VID 0 TMV_RUN_CUSTOMIZABLE_VIEWER 0 TMV_RUN_INTERNAL_DETAILS 1 TMV_RUN_INTERNAL_DETAILS_ON_IO 0 TMV_RUN_INTERNAL_DETAILS_ON_IOBUF 1 TMV_RUN_INTERNAL_DETAILS_ON_LCELL 0 TMV_RUN_INTERNAL_DETAILS_ON_LRAM 0 TRANSCEIVER_3G_BLOCK 0 TRANSCEIVER_6G_BLOCK 0 USES_ACV_FOR_FLED 1 USES_ADB_FOR_BACK_ANNOTATION 1 USES_ALTERA_LNSIM 0 USES_ASIC_ROUTING_POWER_CALCULATOR 0 USES_DATA_DRIVEN_PLL_COMPUTATION_UTIL 1 USES_DEV 1 USES_ICP_FOR_ECO_FITTER 0 USES_LIBERTY_TIMING 0 USES_NETWORK_ROUTING_POWER_CALCULATOR 0 USES_PART_INFO_FOR_DISPLAYING_CORE_VOLTAGE_VALUE 0 USES_POWER_SIGNAL_ACTIVITIES 1 USES_PVAFAM2 0 USES_SECOND_GENERATION_PART_INFO 0 USES_SECOND_GENERATION_POWER_ANALYZER 0 USES_THIRD_GENERATION_TIMING_MODELS_TIS 1 USES_U2B2_TIMING_MODELS 0 USES_XML_FORMAT_FOR_EMIF_PIN_MAP_FILE 0 USE_ADVANCED_IO_POWER_BY_DEFAULT 1 USE_ADVANCED_IO_TIMING_BY_DEFAULT 1 USE_BASE_FAMILY_DDB_PATH 0 USE_OCT_AUTO_CALIBRATION 1 USE_RELAX_IO_ASSIGNMENT_RULES 1 USE_RISEFALL_ONLY 1 USE_SEPARATE_LIST_FOR_TECH_MIGRATION 0 USE_SINGLE_COMPILER_PASS_PLL_MIF_FILE_WRITER 1 USE_TITAN_IO_BASED_IO_REGISTER_PACKER_UTIL 0 USING_28NM_OR_OLDER_TIMING_METHODOLOGY 0 WYSIWYG_BUS_WIDTH_CHECKING_IN_CUT_ENABLED 1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FEATURES</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE">
   <type>java.lang.String</type>
   <value>10M08DAF256C8GES</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE_SPEEDGRADE">
   <type>java.lang.String</type>
   <value>8</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_SPEEDGRADE</sysinfo_type>
  </parameter>
  <parameter name="AUTO_CLK_CLOCK_DOMAIN">
   <type>java.lang.Integer</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_DOMAIN</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="AUTO_CLK_RESET_DOMAIN">
   <type>java.lang.Integer</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>RESET_DOMAIN</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>20000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
   <port>
    <name>reset_req</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
  <interface name="data_master" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>debug.providesServices</name>
    <value>master</value>
   </assignment>
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>d_address</name>
    <direction>Output</direction>
    <width>17</width>
    <role>address</role>
   </port>
   <port>
    <name>d_byteenable</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>d_read</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>d_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>d_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>d_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>d_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>debug_mem_slave_debugaccess_to_roms</name>
    <direction>Output</direction>
    <width>1</width>
    <role>debugaccess</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_0</moduleName>
    <slaveName>nios2_gen2_0_data_master</slaveName>
    <name>mm_interconnect_0.nios2_gen2_0_data_master</name>
    <baseAddress>0</baseAddress>
    <span>131072</span>
   </memoryBlock>
  </interface>
  <interface name="instruction_master" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>i_address</name>
    <direction>Output</direction>
    <width>17</width>
    <role>address</role>
   </port>
   <port>
    <name>i_read</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>i_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>i_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>mm_interconnect_0</moduleName>
    <slaveName>nios2_gen2_0_instruction_master</slaveName>
    <name>mm_interconnect_0.nios2_gen2_0_instruction_master</name>
    <baseAddress>0</baseAddress>
    <span>131072</span>
   </memoryBlock>
  </interface>
  <interface name="irq" kind="interrupt_receiver" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedAddressablePoint">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value>nios2_gen2_0.data_master</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqMap">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqScheme">
    <type>com.altera.sopcmodel.interrupt.InterruptConnectionPoint$EIrqScheme</type>
    <value>INDIVIDUAL_REQUESTS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>interrupt</type>
   <isStart>true</isStart>
   <port>
    <name>irq</name>
    <direction>Input</direction>
    <width>32</width>
    <role>irq</role>
   </port>
   <interrupt>
    <isBridge>false</isBridge>
    <moduleName>irq_mapper</moduleName>
    <slaveName>sender</slaveName>
    <name>irq_mapper.sender</name>
    <interruptNumber>0</interruptNumber>
   </interrupt>
  </interface>
  <interface name="debug_reset_request" kind="reset_source" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>none</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>debug_reset_request</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="debug_mem_slave" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.hideDevice</name>
    <value>1</value>
   </assignment>
   <assignment>
    <name>qsys.ui.connect</name>
    <value>instruction_master,data_master</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>2048</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>debug_mem_slave_address</name>
    <direction>Input</direction>
    <width>9</width>
    <role>address</role>
   </port>
   <port>
    <name>debug_mem_slave_byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>debug_mem_slave_debugaccess</name>
    <direction>Input</direction>
    <width>1</width>
    <role>debugaccess</role>
   </port>
   <port>
    <name>debug_mem_slave_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>debug_mem_slave_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>debug_mem_slave_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>debug_mem_slave_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>debug_mem_slave_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
  </interface>
  <interface
     name="custom_instruction_master"
     kind="nios_custom_instruction_master"
     version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="CIName">
    <type>java.lang.String</type>
    <value></value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressWidth">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockCycle">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="enabled">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="opcodeExtension">
    <type>int</type>
    <value>0</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="sharedCombinationalAndMulticycle">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>nios_custom_instruction</type>
   <isStart>true</isStart>
   <port>
    <name>dummy_ci_port</name>
    <direction>Output</direction>
    <width>1</width>
    <role>readra</role>
   </port>
  </interface>
 </module>
 <module
   name="onchip_memory2_0"
   kind="altera_avalon_onchip_memory2"
   version="16.0"
   path="onchip_memory2_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>embeddedsw.CMacro.ALLOW_IN_SYSTEM_MEMORY_CONTENT_EDITOR</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.ALLOW_MRAM_SIM_CONTENTS_ONLY_FILE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CONTENTS_INFO</name>
   <value>""</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DUAL_PORT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.GUI_RAM_BLOCK_TYPE</name>
   <value>AUTO</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INIT_CONTENTS_FILE</name>
   <value>NIOS_LED_onchip_memory2_0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INIT_MEM_CONTENT</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.INSTANCE_ID</name>
   <value>NONE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.NON_DEFAULT_INIT_FILE_ENABLED</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.RAM_BLOCK_TYPE</name>
   <value>AUTO</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.READ_DURING_WRITE_MODE</name>
   <value>DONT_CARE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SINGLE_CLOCK_OP</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SIZE_MULTIPLE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SIZE_VALUE</name>
   <value>32768</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.WRITABLE</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.DAT_SYM_INSTALL_DIR</name>
   <value>SIM_DIR</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.GENERATE_DAT_SYM</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.GENERATE_HEX</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.HAS_BYTE_LANE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.HEX_INSTALL_DIR</name>
   <value>QPF_DIR</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.MEM_INIT_DATA_WIDTH</name>
   <value>32</value>
  </assignment>
  <assignment>
   <name>embeddedsw.memoryInfo.MEM_INIT_FILENAME</name>
   <value>NIOS_LED_onchip_memory2_0</value>
  </assignment>
  <assignment>
   <name>postgeneration.simulation.init_file.param_name</name>
   <value>INIT_FILE</value>
  </assignment>
  <assignment>
   <name>postgeneration.simulation.init_file.type</name>
   <value>MEM_INIT</value>
  </assignment>
  <parameter name="allowInSystemMemoryContentEditor">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="blockType">
   <type>java.lang.String</type>
   <value>AUTO</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dataWidth">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dataWidth2">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="dualPort">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="enableDiffWidth">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="initMemContent">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="initializationFileName">
   <type>java.lang.String</type>
   <value>onchip_mem.hex</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="instanceID">
   <type>java.lang.String</type>
   <value>NONE</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="memorySize">
   <type>long</type>
   <value>32768</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="readDuringWriteMode">
   <type>java.lang.String</type>
   <value>DONT_CARE</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simAllowMRAMContentsFile">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simMemInitOnlyFilename">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="singleClockOperation">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slave1Latency">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slave2Latency">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="useNonDefaultInitFile">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="copyInitFile">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="useShallowMemBlocks">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="writable">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ecc_enabled">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetrequest_enabled">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="autoInitializationFileName">
   <type>java.lang.String</type>
   <value>NIOS_LED_onchip_memory2_0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>UNIQUE_ID</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>MAX10FPGA</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="deviceFeatures">
   <type>java.lang.String</type>
   <value>ADDRESS_STALL 1 ADVANCED_INFO 0 ALLOWS_COMPILING_OTHER_FAMILY_IP 1 ANY_QFP 0 CELL_LEVEL_BACK_ANNOTATION_DISABLED 0 COMPILER_SUPPORT 1 DSP 1 DSP_SHIFTER_BLOCK 0 DUMP_ASM_LAB_BITS_FOR_POWER 1 EMUL 0 ENABLE_ADVANCED_IO_ANALYSIS_GUI_FEATURES 0 ENABLE_PHYSICAL_DESIGN_PLANNER 0 ENABLE_PIN_PLANNER 0 ENGINEERING_SAMPLE 0 EPCS 1 ESB 0 FAKE1 0 FAKE2 0 FAKE3 0 FAMILY_LEVEL_INSTALLATION_ONLY 0 FASTEST 0 FINAL_TIMING_MODEL 0 FITTER_USE_FALLING_EDGE_DELAY 1 FPP_COMPLETELY_PLACES_AND_ROUTES_PERIPHERY 0 GENERATE_DC_ON_CURRENT_WARNING_FOR_INTERNAL_CLAMPING_DIODE 0 HARDCOPY 0 HAS_18_BIT_MULTS 0 HAS_ACE_SUPPORT 1 HAS_ACTIVE_PARALLEL_FLASH_SUPPORT 0 HAS_ADJUSTABLE_OUTPUT_IO_TIMING_MEAS_POINT 1 HAS_ADVANCED_IO_INVERTED_CORNER 0 HAS_ADVANCED_IO_POWER_SUPPORT 1 HAS_ADVANCED_IO_TIMING_SUPPORT 1 HAS_ALM_SUPPORT 0 HAS_ATOM_AND_ROUTING_POWER_MODELED_TOGETHER 0 HAS_AUTO_DERIVE_CLOCK_UNCERTAINTY_SUPPORT 0 HAS_AUTO_FIT_SUPPORT 1 HAS_BALANCED_OPT_TECHNIQUE_SUPPORT 1 HAS_BENEFICIAL_SKEW_SUPPORT 1 HAS_BITLEVEL_DRIVE_STRENGTH_CONTROL 0 HAS_BSDL_FILE_GENERATION 0 HAS_CDB_RE_NETWORK_PRESERVATION_SUPPORT 0 HAS_CGA_SUPPORT 1 HAS_CHECK_NETLIST_SUPPORT 0 HAS_CLOCK_REGION_CHECKER_ENABLED 1 HAS_CORE_JUNCTION_TEMP_DERATING 0 HAS_CROSSTALK_SUPPORT 0 HAS_CUSTOM_REGION_SUPPORT 1 HAS_DAP_JTAG_FROM_HPS 0 HAS_DATA_DRIVEN_ACVQ_HSSI_SUPPORT 0 HAS_DDB_FDI_SUPPORT 0 HAS_DESIGN_ANALYZER_SUPPORT 0 HAS_DETAILED_IO_RAIL_POWER_MODEL 1 HAS_DETAILED_LEIM_STATIC_POWER_MODEL 0 HAS_DETAILED_LE_POWER_MODEL 1 HAS_DETAILED_ROUTING_MUX_STATIC_POWER_MODEL 0 HAS_DETAILED_THERMAL_CIRCUIT_PARAMETER_SUPPORT 1 HAS_DEVICE_MIGRATION_SUPPORT 1 HAS_DIAGONAL_MIGRATION_SUPPORT 0 HAS_EMIF_TOOLKIT_SUPPORT 0 HAS_ERROR_DETECTION_SUPPORT 0 HAS_FAMILY_VARIANT_MIGRATION_SUPPORT 0 HAS_FANOUT_FREE_NODE_SUPPORT 1 HAS_FAST_FIT_SUPPORT 1 HAS_FITTER_ECO_SUPPORT 1 HAS_FIT_NETLIST_OPT_RETIME_SUPPORT 1 HAS_FIT_NETLIST_OPT_SUPPORT 1 HAS_FORMAL_VERIFICATION_SUPPORT 0 HAS_FPGA_XCHANGE_SUPPORT 0 HAS_FSAC_LUTRAM_REGISTER_PACKING_SUPPORT 0 HAS_FULL_DAT_MIN_TIMING_SUPPORT 1 HAS_FULL_INCREMENTAL_DESIGN_SUPPORT 1 HAS_FUNCTIONAL_SIMULATION_SUPPORT 1 HAS_FUNCTIONAL_VERILOG_SIMULATION_SUPPORT 0 HAS_FUNCTIONAL_VHDL_SIMULATION_SUPPORT 0 HAS_GLITCH_FILTERING_SUPPORT 1 HAS_HARDCOPYII_SUPPORT 0 HAS_HC_READY_SUPPORT 0 HAS_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_HOLD_TIME_AVOIDANCE_ACROSS_CLOCK_SPINE_SUPPORT 1 HAS_HSPICE_WRITER_SUPPORT 0 HAS_HSSI_POWER_CALCULATOR 1 HAS_IBISO_WRITER_SUPPORT 0 HAS_ICD_DATA_IP 0 HAS_IDB_SUPPORT 0 HAS_INCREMENTAL_DAT_SUPPORT 1 HAS_INCREMENTAL_SYNTHESIS_SUPPORT 1 HAS_IO_ASSIGNMENT_ANALYSIS_SUPPORT 1 HAS_IO_DECODER 0 HAS_IO_PLACEMENT_OPTIMIZATION_SUPPORT 1 HAS_IO_PLACEMENT_USING_GEOMETRY_RULE 0 HAS_IO_PLACEMENT_USING_PHYSIC_RULE 0 HAS_IO_SMART_RECOMPILE_SUPPORT 0 HAS_JITTER_SUPPORT 1 HAS_JTAG_SLD_HUB_SUPPORT 1 HAS_LOGIC_LOCK_SUPPORT 1 HAS_MICROPROCESSOR 0 HAS_MIF_SMART_COMPILE_SUPPORT 1 HAS_MINMAX_TIMING_MODELING_SUPPORT 1 HAS_MIN_TIMING_ANALYSIS_SUPPORT 1 HAS_MUX_RESTRUCTURE_SUPPORT 1 HAS_NADDER_STYLE_CLOCKING 0 HAS_NADDER_STYLE_FF 0 HAS_NADDER_STYLE_LCELL_COMB 0 HAS_NEW_CDB_NAME_FOR_M20K_SCLR 0 HAS_NEW_HC_FLOW_SUPPORT 0 HAS_NEW_SERDES_MAX_RESOURCE_COUNT_REPORTING_SUPPORT 1 HAS_NEW_VPR_SUPPORT 1 HAS_NONSOCKET_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_NO_HARDBLOCK_PARTITION_SUPPORT 0 HAS_NO_JTAG_USERCODE_SUPPORT 0 HAS_OPERATING_SETTINGS_AND_CONDITIONS_REPORTING_SUPPORT 1 HAS_PAD_LOCATION_ASSIGNMENT_SUPPORT 0 HAS_PARTIAL_RECONFIG_SUPPORT 0 HAS_PASSIVE_PARALLEL_SUPPORT 0 HAS_PHYSICAL_DESIGN_PLANNER_SUPPORT 0 HAS_PHYSICAL_NETLIST_OUTPUT 0 HAS_PHYSICAL_ROUTING_SUPPORT 0 HAS_PIN_SPECIFIC_VOLTAGE_SUPPORT 1 HAS_PLDM_REF_SUPPORT 0 HAS_POWER_BINNING_LIMITS_DATA 1 HAS_POWER_ESTIMATION_SUPPORT 1 HAS_PRELIMINARY_CLOCK_UNCERTAINTY_NUMBERS 0 HAS_PRE_FITTER_FPP_SUPPORT 0 HAS_PRE_FITTER_LUTRAM_NETLIST_CHECKER_ENABLED 0 HAS_PVA_SUPPORT 1 HAS_QUARTUS_HIERARCHICAL_DESIGN_SUPPORT 0 HAS_RAPID_RECOMPILE_SUPPORT 0 HAS_RCF_SUPPORT 1 HAS_RCF_SUPPORT_FOR_DEBUGGING 0 HAS_RED_BLACK_SEPARATION_SUPPORT 0 HAS_RE_LEVEL_TIMING_GRAPH_SUPPORT 1 HAS_RISEFALL_DELAY_SUPPORT 1 HAS_SIGNAL_PROBE_SUPPORT 1 HAS_SIGNAL_TAP_SUPPORT 1 HAS_SIMULATOR_SUPPORT 0 HAS_SPLIT_IO_SUPPORT 1 HAS_SPLIT_LC_SUPPORT 1 HAS_STRICT_PRESERVATION_SUPPORT 1 HAS_SYNTHESIS_ON_ATOMS 0 HAS_SYNTH_FSYN_NETLIST_OPT_SUPPORT 1 HAS_SYNTH_NETLIST_OPT_RETIME_SUPPORT 0 HAS_SYNTH_NETLIST_OPT_SUPPORT 1 HAS_TCL_FITTER_SUPPORT 0 HAS_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_TEMPLATED_REGISTER_PACKING_SUPPORT 1 HAS_TIME_BORROWING_SUPPORT 0 HAS_TIMING_DRIVEN_SYNTHESIS_SUPPORT 1 HAS_TIMING_INFO_SUPPORT 1 HAS_TIMING_OPERATING_CONDITIONS 1 HAS_TIMING_SIMULATION_SUPPORT 0 HAS_TITAN_BASED_MAC_REGISTER_PACKER_SUPPORT 0 HAS_U2B2_SUPPORT 0 HAS_USER_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_USE_FITTER_INFO_SUPPORT 1 HAS_VCCPD_POWER_RAIL 0 HAS_VERTICAL_MIGRATION_SUPPORT 1 HAS_VIEWDRAW_SYMBOL_SUPPORT 0 HAS_VIO_SUPPORT 1 HAS_VIRTUAL_DEVICES 0 HAS_WYSIWYG_DFFEAS_SUPPORT 1 HAS_XIBISO2_WRITER_SUPPORT 1 HAS_XIBISO_WRITER_SUPPORT 0 IFP_USE_LEGACY_IO_CHECKER 0 INCREMENTAL_DESIGN_SUPPORTS_COMPATIBLE_CONSTRAINTS 1 INSTALLED 0 INTERNAL_POF_SUPPORT_ENABLED 0 INTERNAL_USE_ONLY 0 ISSUE_MILITARY_TEMPERATURE_WARNING 0 IS_CONFIG_ROM 0 IS_DEFAULT_FAMILY 0 IS_FOR_INTERNAL_TESTING_ONLY 0 IS_HARDCOPY_FAMILY 0 IS_HBGA_PACKAGE 0 IS_HIGH_CURRENT_PART 0 IS_LOW_POWER_PART 0 IS_SDM_ONLY_PACKAGE 0 IS_SMI_PART 0 LOAD_BLK_TYPE_DATA_FROM_ATOM_WYS_INFO 0 LVDS_IO 0 M10K_MEMORY 0 M144K_MEMORY 0 M20K_MEMORY 0 M4K_MEMORY 0 M512_MEMORY 0 M9K_MEMORY 1 MLAB_MEMORY 0 MRAM_MEMORY 0 NOT_LISTED 0 NOT_MIGRATABLE 0 NO_FITTER_DELAY_CACHE_GENERATED 0 NO_PIN_OUT 0 NO_POF 0 NO_RPE_SUPPORT 0 NO_SUPPORT_FOR_LOGICLOCK_CONTENT_BACK_ANNOTATION 0 NO_SUPPORT_FOR_STA_CLOCK_UNCERTAINTY_CHECK 0 NO_TDC_SUPPORT 0 POSTFIT_BAK_DATABASE_EXPORT_ENABLED 0 POSTMAP_BAK_DATABASE_EXPORT_ENABLED 0 PROGRAMMER_ONLY 0 PROGRAMMER_SUPPORT 1 PVA_SUPPORTS_ONLY_SUBSET_OF_ATOMS 0 QFIT_IN_DEVELOPMENT 0 QMAP_IN_DEVELOPMENT 0 RAM_LOGICAL_NAME_CHECKING_IN_CUT_ENABLED 1 REPORTS_METASTABILITY_MTBF 1 REQUIRES_INSTALLATION_PATCH 0 REQUIRES_LIST_OF_TEMPERATURE_AND_VOLTAGE_OPERATING_CONDITIONS 1 REQUIRE_QUARTUS_HIERARCHICAL_DESIGN 0 REQUIRE_SPECIAL_HANDLING_FOR_LOCAL_LABLINE 1 RESERVES_SIGNAL_PROBE_PINS 0 RESOLVE_MAX_FANOUT_EARLY 1 RESOLVE_MAX_FANOUT_LATE 0 RESPECTS_FIXED_SIZED_LOCKED_LOCATION_LOGICLOCK 1 RESTRICTED_USER_SELECTION 0 RESTRICT_PARTIAL_RECONFIG 0 RISEFALL_SUPPORT_IS_HIDDEN 0 SHOW_HIDDEN_FAMILY_IN_PROGRAMMER 0 STRICT_TIMING_DB_CHECKS 0 SUPPORTS_ADDITIONAL_OPTIONS_FOR_UNUSED_IO 0 SUPPORTS_CRC 1 SUPPORTS_DIFFERENTIAL_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_DSP_BALANCING_BACK_ANNOTATION 0 SUPPORTS_GENERATION_OF_EARLY_POWER_ESTIMATOR_FILE 1 SUPPORTS_GLOBAL_SIGNAL_BACK_ANNOTATION 0 SUPPORTS_HIPI_RETIMING 0 SUPPORTS_MAC_CHAIN_OUT_ADDER 0 SUPPORTS_RAM_PACKING_BACK_ANNOTATION 0 SUPPORTS_REG_PACKING_BACK_ANNOTATION 0 SUPPORTS_SIGNALPROBE_REGISTER_PIPELINING 1 SUPPORTS_SINGLE_ENDED_AIOT_BOARD_TRACE_MODEL 1 SUPPORTS_USER_MANUAL_LOGIC_DUPLICATION 1 SUPPORTS_VID 0 TMV_RUN_CUSTOMIZABLE_VIEWER 0 TMV_RUN_INTERNAL_DETAILS 1 TMV_RUN_INTERNAL_DETAILS_ON_IO 0 TMV_RUN_INTERNAL_DETAILS_ON_IOBUF 1 TMV_RUN_INTERNAL_DETAILS_ON_LCELL 0 TMV_RUN_INTERNAL_DETAILS_ON_LRAM 0 TRANSCEIVER_3G_BLOCK 0 TRANSCEIVER_6G_BLOCK 0 USES_ACV_FOR_FLED 1 USES_ADB_FOR_BACK_ANNOTATION 1 USES_ALTERA_LNSIM 0 USES_ASIC_ROUTING_POWER_CALCULATOR 0 USES_DATA_DRIVEN_PLL_COMPUTATION_UTIL 1 USES_DEV 1 USES_ICP_FOR_ECO_FITTER 0 USES_LIBERTY_TIMING 0 USES_NETWORK_ROUTING_POWER_CALCULATOR 0 USES_PART_INFO_FOR_DISPLAYING_CORE_VOLTAGE_VALUE 0 USES_POWER_SIGNAL_ACTIVITIES 1 USES_PVAFAM2 0 USES_SECOND_GENERATION_PART_INFO 0 USES_SECOND_GENERATION_POWER_ANALYZER 0 USES_THIRD_GENERATION_TIMING_MODELS_TIS 1 USES_U2B2_TIMING_MODELS 0 USES_XML_FORMAT_FOR_EMIF_PIN_MAP_FILE 0 USE_ADVANCED_IO_POWER_BY_DEFAULT 1 USE_ADVANCED_IO_TIMING_BY_DEFAULT 1 USE_BASE_FAMILY_DDB_PATH 0 USE_OCT_AUTO_CALIBRATION 1 USE_RELAX_IO_ASSIGNMENT_RULES 1 USE_RISEFALL_ONLY 1 USE_SEPARATE_LIST_FOR_TECH_MIGRATION 0 USE_SINGLE_COMPILER_PASS_PLL_MIF_FILE_WRITER 1 USE_TITAN_IO_BASED_IO_REGISTER_PACKER_UTIL 0 USING_28NM_OR_OLDER_TIMING_METHODOLOGY 0 WYSIWYG_BUS_WIDTH_CHECKING_IN_CUT_ENABLED 1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FEATURES</sysinfo_type>
  </parameter>
  <parameter name="derived_set_addr_width">
   <type>int</type>
   <value>13</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_set_addr_width2">
   <type>int</type>
   <value>13</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_set_data_width">
   <type>int</type>
   <value>32</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_set_data_width2">
   <type>int</type>
   <value>32</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_gui_ram_block_type">
   <type>java.lang.String</type>
   <value>Automatic</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_is_hardcopy">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_init_file_name">
   <type>java.lang.String</type>
   <value>NIOS_LED_onchip_memory2_0.hex</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk1" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="s1" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>1</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>32768</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>32768</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>address</name>
    <direction>Input</direction>
    <width>13</width>
    <role>address</role>
   </port>
   <port>
    <name>clken</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <port>
    <name>chipselect</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
  </interface>
  <interface name="reset1" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
 </module>
 <module name="pio_0" kind="altera_avalon_pio" version="16.0" path="pio_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>embeddedsw.CMacro.BIT_CLEARING_EDGE_REGISTER</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.BIT_MODIFYING_OUTPUT_REGISTER</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.CAPTURE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DATA_WIDTH</name>
   <value>4</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DO_TEST_BENCH_WIRING</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.DRIVEN_SIM_VALUE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.EDGE_TYPE</name>
   <value>NONE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FREQ</name>
   <value>20000000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_IN</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_OUT</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.HAS_TRI</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.IRQ_TYPE</name>
   <value>NONE</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.RESET_VALUE</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.compatible</name>
   <value>altr,pio-1.0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.group</name>
   <value>gpio</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.name</name>
   <value>pio</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.altr,gpio-bank-width</name>
   <value>4</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.params.resetvalue</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.vendor</name>
   <value>altr</value>
  </assignment>
  <parameter name="bitClearingEdgeCapReg">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="bitModifyingOutReg">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="captureEdge">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="direction">
   <type>java.lang.String</type>
   <value>Output</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="edgeType">
   <type>java.lang.String</type>
   <value>RISING</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateIRQ">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="irqType">
   <type>java.lang.String</type>
   <value>LEVEL</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetValue">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simDoTestBenchWiring">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="simDrivenValue">
   <type>long</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>false</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="width">
   <type>int</type>
   <value>4</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="clockRate">
   <type>long</type>
   <value>20000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="derived_has_tri">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_has_out">
   <type>boolean</type>
   <value>true</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_has_in">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_do_test_bench_wiring">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_capture">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_edge_type">
   <type>java.lang.String</type>
   <value>NONE</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_irq_type">
   <type>java.lang.String</type>
   <value>NONE</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="derived_has_irq">
   <type>boolean</type>
   <value>false</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>20000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="s1" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>NATIVE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>4</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>address</name>
    <direction>Input</direction>
    <width>2</width>
    <role>address</role>
   </port>
   <port>
    <name>write_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write_n</role>
   </port>
   <port>
    <name>writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>chipselect</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
  </interface>
  <interface name="external_connection" kind="conduit_end" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>conduit</type>
   <isStart>false</isStart>
   <port>
    <name>out_port</name>
    <direction>Output</direction>
    <width>4</width>
    <role>export</role>
   </port>
  </interface>
 </module>
 <module
   name="timer_0"
   kind="altera_avalon_timer"
   version="16.0"
   path="timer_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>embeddedsw.CMacro.ALWAYS_RUN</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.COUNTER_SIZE</name>
   <value>32</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FIXED_PERIOD</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.FREQ</name>
   <value>20000000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.LOAD_VALUE</name>
   <value>4999999</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.MULT</name>
   <value>5e-8</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.PERIOD</name>
   <value>5000000</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.PERIOD_UNITS</name>
   <value>clocks</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.RESET_OUTPUT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.SNAPSHOT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.TICKS_PER_SEC</name>
   <value>4</value>
  </assignment>
  <assignment>
   <name>embeddedsw.CMacro.TIMEOUT_PULSE_OUTPUT</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>embeddedsw.dts.vendor</name>
   <value>altr</value>
  </assignment>
  <parameter name="alwaysRun">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="counterSize">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="fixedPeriod">
   <type>boolean</type>
   <value>true</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="period">
   <type>java.lang.String</type>
   <value>5000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="periodUnits">
   <type>java.lang.String</type>
   <value>CLOCKS</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="resetOutput">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="snapshot">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="timeoutPulseOutput">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="systemFrequency">
   <type>long</type>
   <value>20000000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>CLOCK_RATE</sysinfo_type>
   <sysinfo_arg>clk</sysinfo_arg>
  </parameter>
  <parameter name="watchdogPulse">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="timerPreset">
   <type>java.lang.String</type>
   <value>SIMPLE_PERIODIC_INTERRUPT</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="periodUnitsString">
   <type>java.lang.String</type>
   <value>clocks</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="valueInSecond">
   <type>double</type>
   <value>0.0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="loadValue">
   <type>java.lang.String</type>
   <value>4999999</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="mult">
   <type>double</type>
   <value>5.0E-8</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ticksPerSec">
   <type>double</type>
   <value>4.0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="slave_address_width">
   <type>int</type>
   <value>3</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRateKnown">
    <type>java.lang.Boolean</type>
    <value>true</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="clockRate">
    <type>java.lang.Long</type>
    <value>20000000</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_n</role>
   </port>
  </interface>
  <interface name="s1" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isTimerDevice</name>
    <value>1</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>NATIVE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>8</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>address</name>
    <direction>Input</direction>
    <width>3</width>
    <role>address</role>
   </port>
   <port>
    <name>writedata</name>
    <direction>Input</direction>
    <width>16</width>
    <role>writedata</role>
   </port>
   <port>
    <name>readdata</name>
    <direction>Output</direction>
    <width>16</width>
    <role>readdata</role>
   </port>
   <port>
    <name>chipselect</name>
    <direction>Input</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>write_n</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write_n</role>
   </port>
  </interface>
  <interface name="irq" kind="interrupt_sender" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedAddressablePoint">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value>timer_0.s1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedReceiverOffset">
    <type>java.lang.Integer</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToReceiver">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqScheme">
    <type>com.altera.sopcmodel.interrupt.InterruptConnectionPoint$EIrqScheme</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>interrupt</type>
   <isStart>false</isStart>
   <port>
    <name>irq</name>
    <direction>Output</direction>
    <width>1</width>
    <role>irq</role>
   </port>
  </interface>
 </module>
 <module
   name="mm_interconnect_0"
   kind="altera_mm_interconnect"
   version="16.0"
   path="mm_interconnect_0">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <assignment>
   <name>interconnect_id.hex7led_0.avalon_slave_0</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.nios2_gen2_0.data_master</name>
   <value>0</value>
  </assignment>
  <assignment>
   <name>interconnect_id.nios2_gen2_0.debug_mem_slave</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>interconnect_id.nios2_gen2_0.instruction_master</name>
   <value>1</value>
  </assignment>
  <assignment>
   <name>interconnect_id.onchip_memory2_0.s1</name>
   <value>2</value>
  </assignment>
  <assignment>
   <name>interconnect_id.pio_0.s1</name>
   <value>3</value>
  </assignment>
  <assignment>
   <name>interconnect_id.timer_0.s1</name>
   <value>4</value>
  </assignment>
  <parameter name="COMPOSE_CONTENTS">
   <type>java.lang.String</type>
   <value><![CDATA[add_instance {nios2_gen2_0_data_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_ADDRESS_W} {17};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_DATA_W} {32};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_READDATA} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_READ} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_WRITE} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_DEBUGACCESS} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_LOCK} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_BURSTBOUNDARIES} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_REGISTERINCOMINGSIGNALS} {1};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {nios2_gen2_0_data_master_translator} {SYNC_RESET} {0};add_instance {nios2_gen2_0_instruction_master_translator} {altera_merlin_master_translator};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_ADDRESS_W} {17};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_DATA_W} {32};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_READLATENCY} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_READDATA} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_WRITEDATA} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_READ} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_WRITE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_ADDRESS} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_CLKEN} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_LOCK} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_ADDRESS_SYMBOLS} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_LINEWRAPBURSTS} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {64};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_translator} {SYNC_RESET} {0};add_instance {hex7led_0_avalon_slave_0_translator} {altera_merlin_slave_translator};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_ADDRESS_W} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_DATA_W} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_DATA_W} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_BYTEENABLE_W} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_BYTEENABLE_W} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_BURSTCOUNT_W} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_READLATENCY} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_READDATA} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_READ} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_WRITE} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_ADDRESS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_LOCK} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_SYMBOLS_PER_WORD} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {nios2_gen2_0_debug_mem_slave_translator} {altera_merlin_slave_translator};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_ADDRESS_W} {9};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_DATA_W} {32};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_DATA_W} {32};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_BYTEENABLE_W} {4};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_READLATENCY} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_READDATA} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_READ} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_WRITE} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_CHIPSELECT} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_ADDRESS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_WAITREQUEST} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_LOCK} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_DEBUGACCESS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_REGISTERINCOMINGSIGNALS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {onchip_memory2_0_s1_translator} {altera_merlin_slave_translator};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESS_W} {13};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_DATA_W} {32};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_DATA_W} {32};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BYTEENABLE_W} {4};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_BYTEENABLE_W} {4};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_READLATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_READ_WAIT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READDATA} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READ} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITE} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BYTEENABLE} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_ADDRESS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_LOCK} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_AV_CLKEN} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {onchip_memory2_0_s1_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {timer_0_s1_translator} {altera_merlin_slave_translator};set_instance_parameter_value {timer_0_s1_translator} {AV_ADDRESS_W} {3};set_instance_parameter_value {timer_0_s1_translator} {AV_DATA_W} {16};set_instance_parameter_value {timer_0_s1_translator} {UAV_DATA_W} {32};set_instance_parameter_value {timer_0_s1_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {timer_0_s1_translator} {AV_BYTEENABLE_W} {1};set_instance_parameter_value {timer_0_s1_translator} {UAV_BYTEENABLE_W} {4};set_instance_parameter_value {timer_0_s1_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {timer_0_s1_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {timer_0_s1_translator} {AV_READLATENCY} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {timer_0_s1_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_READDATA} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_READ} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_WRITE} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_ADDRESS} {1};set_instance_parameter_value {timer_0_s1_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_LOCK} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {timer_0_s1_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {timer_0_s1_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {timer_0_s1_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {timer_0_s1_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {timer_0_s1_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {timer_0_s1_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {timer_0_s1_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {timer_0_s1_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {pio_0_s1_translator} {altera_merlin_slave_translator};set_instance_parameter_value {pio_0_s1_translator} {AV_ADDRESS_W} {2};set_instance_parameter_value {pio_0_s1_translator} {AV_DATA_W} {32};set_instance_parameter_value {pio_0_s1_translator} {UAV_DATA_W} {32};set_instance_parameter_value {pio_0_s1_translator} {AV_BURSTCOUNT_W} {1};set_instance_parameter_value {pio_0_s1_translator} {AV_BYTEENABLE_W} {1};set_instance_parameter_value {pio_0_s1_translator} {UAV_BYTEENABLE_W} {4};set_instance_parameter_value {pio_0_s1_translator} {UAV_ADDRESS_W} {17};set_instance_parameter_value {pio_0_s1_translator} {UAV_BURSTCOUNT_W} {3};set_instance_parameter_value {pio_0_s1_translator} {AV_READLATENCY} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_SETUP_WAIT} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_WRITE_WAIT} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_READ_WAIT} {1};set_instance_parameter_value {pio_0_s1_translator} {AV_DATA_HOLD} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_TIMING_UNITS} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_READDATA} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_WRITEDATA} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_READ} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_WRITE} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_BEGINBURSTTRANSFER} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_BEGINTRANSFER} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_BYTEENABLE} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_CHIPSELECT} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_ADDRESS} {1};set_instance_parameter_value {pio_0_s1_translator} {USE_BURSTCOUNT} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_READDATAVALID} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_WAITREQUEST} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_WRITEBYTEENABLE} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_LOCK} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_AV_CLKEN} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_UAV_CLKEN} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_OUTPUTENABLE} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_DEBUGACCESS} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_READRESPONSE} {0};set_instance_parameter_value {pio_0_s1_translator} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_SYMBOLS_PER_WORD} {4};set_instance_parameter_value {pio_0_s1_translator} {AV_ADDRESS_SYMBOLS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pio_0_s1_translator} {UAV_CONSTANT_BURST_BEHAVIOR} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_REQUIRE_UNALIGNED_ADDRESSES} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_MAX_PENDING_READ_TRANSACTIONS} {1};set_instance_parameter_value {pio_0_s1_translator} {AV_MAX_PENDING_WRITE_TRANSACTIONS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_INTERLEAVEBURSTS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_BITS_PER_SYMBOL} {8};set_instance_parameter_value {pio_0_s1_translator} {AV_ISBIGENDIAN} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_ADDRESSGROUP} {0};set_instance_parameter_value {pio_0_s1_translator} {UAV_ADDRESSGROUP} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_REGISTEROUTGOINGSIGNALS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_REGISTERINCOMINGSIGNALS} {0};set_instance_parameter_value {pio_0_s1_translator} {AV_ALWAYSBURSTMAXBURST} {0};set_instance_parameter_value {pio_0_s1_translator} {CHIPSELECT_THROUGH_READLATENCY} {0};add_instance {nios2_gen2_0_data_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_QOS_H} {73};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_QOS_L} {73};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DATA_SIDEBAND_H} {71};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DATA_SIDEBAND_L} {71};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ADDR_SIDEBAND_H} {70};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ADDR_SIDEBAND_L} {70};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURST_TYPE_H} {69};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURST_TYPE_L} {68};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_CACHE_H} {87};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_CACHE_L} {84};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_THREAD_ID_H} {80};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_THREAD_ID_L} {80};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_EXCLUSIVE} {58};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DATA_H} {31};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {ST_DATA_W} {93};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {AV_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {AV_BURSTBOUNDARIES} {1};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="0"
   name="hex7led_0_avalon_slave_0_translator.avalon_universal_slave_0"
   start="0x0000000000011030"
   end="0x00000000000011032"
   responds="0"
   user_default="0" />
 <slave
   id="1"
   name="nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0"
   start="0x0000000000010800"
   end="0x00000000000011000"
   responds="1"
   user_default="0" />
 <slave
   id="2"
   name="onchip_memory2_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000008000"
   end="0x00000000000010000"
   responds="1"
   user_default="0" />
 <slave
   id="4"
   name="timer_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000011000"
   end="0x00000000000011020"
   responds="1"
   user_default="0" />
 <slave
   id="3"
   name="pio_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000011020"
   end="0x00000000000011030"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {SUPPRESS_0_BYTEEN_RSP} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {ID} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {BURSTWRAP_VALUE} {7};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_data_master_agent} {USE_WRITERESPONSE} {0};add_instance {nios2_gen2_0_instruction_master_agent} {altera_merlin_master_agent};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_QOS_H} {73};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_QOS_L} {73};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DATA_SIDEBAND_H} {71};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DATA_SIDEBAND_L} {71};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ADDR_SIDEBAND_H} {70};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ADDR_SIDEBAND_L} {70};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURST_TYPE_H} {69};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURST_TYPE_L} {68};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_CACHE_H} {87};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_CACHE_L} {84};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_THREAD_ID_H} {80};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_THREAD_ID_L} {80};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_EXCLUSIVE} {58};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DATA_H} {31};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DATA_L} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {ST_DATA_W} {93};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {AV_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {AV_LINEWRAPBURSTS} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {AV_BURSTBOUNDARIES} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {ADDR_MAP} {<?xml version="1.0" encoding="UTF-8"?>
<address_map>
 <slave
   id="2"
   name="onchip_memory2_0_s1_translator.avalon_universal_slave_0"
   start="0x0000000000008000"
   end="0x00000000000010000"
   responds="1"
   user_default="0" />
 <slave
   id="1"
   name="nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0"
   start="0x0000000000010800"
   end="0x00000000000011000"
   responds="1"
   user_default="0" />
</address_map>
};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {SUPPRESS_0_BYTEEN_RSP} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {ID} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {BURSTWRAP_VALUE} {3};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {CACHE_VALUE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {SECURE_ACCESS_BIT} {1};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_instruction_master_agent} {USE_WRITERESPONSE} {0};add_instance {hex7led_0_avalon_slave_0_agent} {altera_merlin_slave_agent};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_ORI_BURST_SIZE_H} {74};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_ORI_BURST_SIZE_L} {72};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_RESPONSE_STATUS_H} {71};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_RESPONSE_STATUS_L} {70};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BURST_SIZE_H} {49};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BURST_SIZE_L} {47};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_TRANS_LOCK} {39};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BEGIN_BURST} {54};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_PROTECTION_H} {65};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_PROTECTION_L} {63};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BURSTWRAP_H} {46};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BURSTWRAP_L} {44};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BYTE_CNT_H} {43};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BYTE_CNT_L} {41};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_ADDR_H} {34};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_ADDR_L} {18};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_TRANS_COMPRESSED_READ} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_TRANS_POSTED} {36};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_TRANS_WRITE} {37};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_TRANS_READ} {38};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_DATA_H} {15};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_DATA_L} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BYTEEN_H} {17};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_BYTEEN_L} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_SRC_ID_H} {58};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_SRC_ID_L} {56};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_DEST_ID_H} {61};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_DEST_ID_L} {59};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {ST_DATA_W} {75};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {AVS_BURSTCOUNT_W} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(74:72) response_status(71:70) cache(69:66) protection(65:63) thread_id(62) dest_id(61:59) src_id(58:56) qos(55) begin_burst(54) data_sideband(53) addr_sideband(52) burst_type(51:50) burst_size(49:47) burstwrap(46:44) byte_cnt(43:41) trans_exclusive(40) trans_lock(39) trans_read(38) trans_write(37) trans_posted(36) trans_compressed_read(35) addr(34:18) byteen(17:16) data(15:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {SUPPRESS_0_BYTEEN_CMD} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {MAX_BYTE_CNT} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {MAX_BURSTWRAP} {7};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {ID} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {USE_WRITERESPONSE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent} {ECC_ENABLE} {0};add_instance {hex7led_0_avalon_slave_0_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {BITS_PER_SYMBOL} {76};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {hex7led_0_avalon_slave_0_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {nios2_gen2_0_debug_mem_slave_agent} {altera_merlin_slave_agent};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_DATA_H} {31};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_DATA_L} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {ST_DATA_W} {93};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {AVS_BURSTCOUNT_W} {3};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {MAX_BYTE_CNT} {4};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {MAX_BURSTWRAP} {7};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {ID} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {USE_WRITERESPONSE} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent} {ECC_ENABLE} {0};add_instance {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {BITS_PER_SYMBOL} {94};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {onchip_memory2_0_s1_agent} {altera_merlin_slave_agent};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DATA_H} {31};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DATA_L} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ST_DATA_W} {93};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AVS_BURSTCOUNT_W} {3};set_instance_parameter_value {onchip_memory2_0_s1_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {onchip_memory2_0_s1_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MAX_BYTE_CNT} {4};set_instance_parameter_value {onchip_memory2_0_s1_agent} {MAX_BURSTWRAP} {7};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ID} {2};set_instance_parameter_value {onchip_memory2_0_s1_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {USE_WRITERESPONSE} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent} {ECC_ENABLE} {0};add_instance {onchip_memory2_0_s1_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {BITS_PER_SYMBOL} {94};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {onchip_memory2_0_s1_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {timer_0_s1_agent} {altera_merlin_slave_agent};set_instance_parameter_value {timer_0_s1_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {timer_0_s1_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {timer_0_s1_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {timer_0_s1_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {timer_0_s1_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {timer_0_s1_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {timer_0_s1_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {timer_0_s1_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {timer_0_s1_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {timer_0_s1_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {timer_0_s1_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {timer_0_s1_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {timer_0_s1_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {timer_0_s1_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {timer_0_s1_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {timer_0_s1_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {timer_0_s1_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {timer_0_s1_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {timer_0_s1_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {timer_0_s1_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {timer_0_s1_agent} {PKT_DATA_H} {31};set_instance_parameter_value {timer_0_s1_agent} {PKT_DATA_L} {0};set_instance_parameter_value {timer_0_s1_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {timer_0_s1_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {timer_0_s1_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {timer_0_s1_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {timer_0_s1_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {timer_0_s1_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {timer_0_s1_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {timer_0_s1_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {timer_0_s1_agent} {ST_DATA_W} {93};set_instance_parameter_value {timer_0_s1_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {timer_0_s1_agent} {AVS_BURSTCOUNT_W} {3};set_instance_parameter_value {timer_0_s1_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {timer_0_s1_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {timer_0_s1_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {timer_0_s1_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {timer_0_s1_agent} {MAX_BYTE_CNT} {4};set_instance_parameter_value {timer_0_s1_agent} {MAX_BURSTWRAP} {7};set_instance_parameter_value {timer_0_s1_agent} {ID} {4};set_instance_parameter_value {timer_0_s1_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {timer_0_s1_agent} {USE_WRITERESPONSE} {0};set_instance_parameter_value {timer_0_s1_agent} {ECC_ENABLE} {0};add_instance {timer_0_s1_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {BITS_PER_SYMBOL} {94};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {timer_0_s1_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {pio_0_s1_agent} {altera_merlin_slave_agent};set_instance_parameter_value {pio_0_s1_agent} {PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {pio_0_s1_agent} {PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {pio_0_s1_agent} {PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {pio_0_s1_agent} {PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {pio_0_s1_agent} {PKT_BURST_SIZE_H} {67};set_instance_parameter_value {pio_0_s1_agent} {PKT_BURST_SIZE_L} {65};set_instance_parameter_value {pio_0_s1_agent} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {pio_0_s1_agent} {PKT_BEGIN_BURST} {72};set_instance_parameter_value {pio_0_s1_agent} {PKT_PROTECTION_H} {83};set_instance_parameter_value {pio_0_s1_agent} {PKT_PROTECTION_L} {81};set_instance_parameter_value {pio_0_s1_agent} {PKT_BURSTWRAP_H} {64};set_instance_parameter_value {pio_0_s1_agent} {PKT_BURSTWRAP_L} {62};set_instance_parameter_value {pio_0_s1_agent} {PKT_BYTE_CNT_H} {61};set_instance_parameter_value {pio_0_s1_agent} {PKT_BYTE_CNT_L} {59};set_instance_parameter_value {pio_0_s1_agent} {PKT_ADDR_H} {52};set_instance_parameter_value {pio_0_s1_agent} {PKT_ADDR_L} {36};set_instance_parameter_value {pio_0_s1_agent} {PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {pio_0_s1_agent} {PKT_TRANS_POSTED} {54};set_instance_parameter_value {pio_0_s1_agent} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {pio_0_s1_agent} {PKT_TRANS_READ} {56};set_instance_parameter_value {pio_0_s1_agent} {PKT_DATA_H} {31};set_instance_parameter_value {pio_0_s1_agent} {PKT_DATA_L} {0};set_instance_parameter_value {pio_0_s1_agent} {PKT_BYTEEN_H} {35};set_instance_parameter_value {pio_0_s1_agent} {PKT_BYTEEN_L} {32};set_instance_parameter_value {pio_0_s1_agent} {PKT_SRC_ID_H} {76};set_instance_parameter_value {pio_0_s1_agent} {PKT_SRC_ID_L} {74};set_instance_parameter_value {pio_0_s1_agent} {PKT_DEST_ID_H} {79};set_instance_parameter_value {pio_0_s1_agent} {PKT_DEST_ID_L} {77};set_instance_parameter_value {pio_0_s1_agent} {PKT_SYMBOL_W} {8};set_instance_parameter_value {pio_0_s1_agent} {ST_CHANNEL_W} {5};set_instance_parameter_value {pio_0_s1_agent} {ST_DATA_W} {93};set_instance_parameter_value {pio_0_s1_agent} {AVS_BURSTCOUNT_SYMBOLS} {0};set_instance_parameter_value {pio_0_s1_agent} {AVS_BURSTCOUNT_W} {3};set_instance_parameter_value {pio_0_s1_agent} {AV_LINEWRAPBURSTS} {0};set_instance_parameter_value {pio_0_s1_agent} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {pio_0_s1_agent} {SUPPRESS_0_BYTEEN_CMD} {0};set_instance_parameter_value {pio_0_s1_agent} {PREVENT_FIFO_OVERFLOW} {1};set_instance_parameter_value {pio_0_s1_agent} {MAX_BYTE_CNT} {4};set_instance_parameter_value {pio_0_s1_agent} {MAX_BURSTWRAP} {7};set_instance_parameter_value {pio_0_s1_agent} {ID} {3};set_instance_parameter_value {pio_0_s1_agent} {USE_READRESPONSE} {0};set_instance_parameter_value {pio_0_s1_agent} {USE_WRITERESPONSE} {0};set_instance_parameter_value {pio_0_s1_agent} {ECC_ENABLE} {0};add_instance {pio_0_s1_agent_rsp_fifo} {altera_avalon_sc_fifo};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {SYMBOLS_PER_BEAT} {1};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {BITS_PER_SYMBOL} {94};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {FIFO_DEPTH} {2};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {CHANNEL_WIDTH} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {ERROR_WIDTH} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_PACKETS} {1};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_FILL_LEVEL} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {EMPTY_LATENCY} {1};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_MEMORY_BLOCKS} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_STORE_FORWARD} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_ALMOST_FULL_IF} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {USE_ALMOST_EMPTY_IF} {0};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {ENABLE_EXPLICIT_MAXCHANNEL} {false};set_instance_parameter_value {pio_0_s1_agent_rsp_fifo} {EXPLICIT_MAXCHANNEL} {0};add_instance {router} {altera_merlin_router};set_instance_parameter_value {router} {DESTINATION_ID} {2 1 4 3 0 };set_instance_parameter_value {router} {CHANNEL_ID} {00100 00010 01000 10000 00001 };set_instance_parameter_value {router} {TYPE_OF_TRANSACTION} {both both both both write };set_instance_parameter_value {router} {START_ADDRESS} {0x8000 0x10800 0x11000 0x11020 0x11030 };set_instance_parameter_value {router} {END_ADDRESS} {0x10000 0x11000 0x11020 0x11030 0x11032 };set_instance_parameter_value {router} {NON_SECURED_TAG} {1 1 1 1 1 };set_instance_parameter_value {router} {SECURED_RANGE_PAIRS} {0 0 0 0 0 };set_instance_parameter_value {router} {SECURED_RANGE_LIST} {0 0 0 0 0 };set_instance_parameter_value {router} {SPAN_OFFSET} {};set_instance_parameter_value {router} {PKT_ADDR_H} {52};set_instance_parameter_value {router} {PKT_ADDR_L} {36};set_instance_parameter_value {router} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router} {PKT_TRANS_READ} {56};set_instance_parameter_value {router} {ST_DATA_W} {93};set_instance_parameter_value {router} {ST_CHANNEL_W} {5};set_instance_parameter_value {router} {DECODER_TYPE} {0};set_instance_parameter_value {router} {DEFAULT_CHANNEL} {2};set_instance_parameter_value {router} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router} {DEFAULT_DESTID} {2};set_instance_parameter_value {router} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router} {MEMORY_ALIASING_DECODE} {0};add_instance {router_001} {altera_merlin_router};set_instance_parameter_value {router_001} {DESTINATION_ID} {2 1 };set_instance_parameter_value {router_001} {CHANNEL_ID} {10 01 };set_instance_parameter_value {router_001} {TYPE_OF_TRANSACTION} {both both };set_instance_parameter_value {router_001} {START_ADDRESS} {0x8000 0x10800 };set_instance_parameter_value {router_001} {END_ADDRESS} {0x10000 0x11000 };set_instance_parameter_value {router_001} {NON_SECURED_TAG} {1 1 };set_instance_parameter_value {router_001} {SECURED_RANGE_PAIRS} {0 0 };set_instance_parameter_value {router_001} {SECURED_RANGE_LIST} {0 0 };set_instance_parameter_value {router_001} {SPAN_OFFSET} {};set_instance_parameter_value {router_001} {PKT_ADDR_H} {52};set_instance_parameter_value {router_001} {PKT_ADDR_L} {36};set_instance_parameter_value {router_001} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router_001} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router_001} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router_001} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router_001} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router_001} {PKT_TRANS_READ} {56};set_instance_parameter_value {router_001} {ST_DATA_W} {93};set_instance_parameter_value {router_001} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_001} {DECODER_TYPE} {0};set_instance_parameter_value {router_001} {DEFAULT_CHANNEL} {1};set_instance_parameter_value {router_001} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_001} {DEFAULT_DESTID} {2};set_instance_parameter_value {router_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_001} {MEMORY_ALIASING_DECODE} {0};add_instance {router_002} {altera_merlin_router};set_instance_parameter_value {router_002} {DESTINATION_ID} {0 };set_instance_parameter_value {router_002} {CHANNEL_ID} {1 };set_instance_parameter_value {router_002} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router_002} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_002} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_002} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_002} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_002} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_002} {SPAN_OFFSET} {};set_instance_parameter_value {router_002} {PKT_ADDR_H} {34};set_instance_parameter_value {router_002} {PKT_ADDR_L} {18};set_instance_parameter_value {router_002} {PKT_PROTECTION_H} {65};set_instance_parameter_value {router_002} {PKT_PROTECTION_L} {63};set_instance_parameter_value {router_002} {PKT_DEST_ID_H} {61};set_instance_parameter_value {router_002} {PKT_DEST_ID_L} {59};set_instance_parameter_value {router_002} {PKT_TRANS_WRITE} {37};set_instance_parameter_value {router_002} {PKT_TRANS_READ} {38};set_instance_parameter_value {router_002} {ST_DATA_W} {75};set_instance_parameter_value {router_002} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_002} {DECODER_TYPE} {1};set_instance_parameter_value {router_002} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_002} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_002} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(74:72) response_status(71:70) cache(69:66) protection(65:63) thread_id(62) dest_id(61:59) src_id(58:56) qos(55) begin_burst(54) data_sideband(53) addr_sideband(52) burst_type(51:50) burst_size(49:47) burstwrap(46:44) byte_cnt(43:41) trans_exclusive(40) trans_lock(39) trans_read(38) trans_write(37) trans_posted(36) trans_compressed_read(35) addr(34:18) byteen(17:16) data(15:0)};set_instance_parameter_value {router_002} {MEMORY_ALIASING_DECODE} {0};add_instance {router_003} {altera_merlin_router};set_instance_parameter_value {router_003} {DESTINATION_ID} {0 1 };set_instance_parameter_value {router_003} {CHANNEL_ID} {01 10 };set_instance_parameter_value {router_003} {TYPE_OF_TRANSACTION} {both read };set_instance_parameter_value {router_003} {START_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_003} {END_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_003} {NON_SECURED_TAG} {1 1 };set_instance_parameter_value {router_003} {SECURED_RANGE_PAIRS} {0 0 };set_instance_parameter_value {router_003} {SECURED_RANGE_LIST} {0 0 };set_instance_parameter_value {router_003} {SPAN_OFFSET} {};set_instance_parameter_value {router_003} {PKT_ADDR_H} {52};set_instance_parameter_value {router_003} {PKT_ADDR_L} {36};set_instance_parameter_value {router_003} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router_003} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router_003} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router_003} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router_003} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router_003} {PKT_TRANS_READ} {56};set_instance_parameter_value {router_003} {ST_DATA_W} {93};set_instance_parameter_value {router_003} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_003} {DECODER_TYPE} {1};set_instance_parameter_value {router_003} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_003} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_003} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_003} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_003} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_003} {MEMORY_ALIASING_DECODE} {0};add_instance {router_004} {altera_merlin_router};set_instance_parameter_value {router_004} {DESTINATION_ID} {0 1 };set_instance_parameter_value {router_004} {CHANNEL_ID} {01 10 };set_instance_parameter_value {router_004} {TYPE_OF_TRANSACTION} {both read };set_instance_parameter_value {router_004} {START_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_004} {END_ADDRESS} {0x0 0x0 };set_instance_parameter_value {router_004} {NON_SECURED_TAG} {1 1 };set_instance_parameter_value {router_004} {SECURED_RANGE_PAIRS} {0 0 };set_instance_parameter_value {router_004} {SECURED_RANGE_LIST} {0 0 };set_instance_parameter_value {router_004} {SPAN_OFFSET} {};set_instance_parameter_value {router_004} {PKT_ADDR_H} {52};set_instance_parameter_value {router_004} {PKT_ADDR_L} {36};set_instance_parameter_value {router_004} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router_004} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router_004} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router_004} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router_004} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router_004} {PKT_TRANS_READ} {56};set_instance_parameter_value {router_004} {ST_DATA_W} {93};set_instance_parameter_value {router_004} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_004} {DECODER_TYPE} {1};set_instance_parameter_value {router_004} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_004} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_004} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_004} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_004} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_004} {MEMORY_ALIASING_DECODE} {0};add_instance {router_005} {altera_merlin_router};set_instance_parameter_value {router_005} {DESTINATION_ID} {0 };set_instance_parameter_value {router_005} {CHANNEL_ID} {1 };set_instance_parameter_value {router_005} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router_005} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_005} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_005} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_005} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_005} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_005} {SPAN_OFFSET} {};set_instance_parameter_value {router_005} {PKT_ADDR_H} {52};set_instance_parameter_value {router_005} {PKT_ADDR_L} {36};set_instance_parameter_value {router_005} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router_005} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router_005} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router_005} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router_005} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router_005} {PKT_TRANS_READ} {56};set_instance_parameter_value {router_005} {ST_DATA_W} {93};set_instance_parameter_value {router_005} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_005} {DECODER_TYPE} {1};set_instance_parameter_value {router_005} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_005} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_005} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_005} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_005} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_005} {MEMORY_ALIASING_DECODE} {0};add_instance {router_006} {altera_merlin_router};set_instance_parameter_value {router_006} {DESTINATION_ID} {0 };set_instance_parameter_value {router_006} {CHANNEL_ID} {1 };set_instance_parameter_value {router_006} {TYPE_OF_TRANSACTION} {both };set_instance_parameter_value {router_006} {START_ADDRESS} {0x0 };set_instance_parameter_value {router_006} {END_ADDRESS} {0x0 };set_instance_parameter_value {router_006} {NON_SECURED_TAG} {1 };set_instance_parameter_value {router_006} {SECURED_RANGE_PAIRS} {0 };set_instance_parameter_value {router_006} {SECURED_RANGE_LIST} {0 };set_instance_parameter_value {router_006} {SPAN_OFFSET} {};set_instance_parameter_value {router_006} {PKT_ADDR_H} {52};set_instance_parameter_value {router_006} {PKT_ADDR_L} {36};set_instance_parameter_value {router_006} {PKT_PROTECTION_H} {83};set_instance_parameter_value {router_006} {PKT_PROTECTION_L} {81};set_instance_parameter_value {router_006} {PKT_DEST_ID_H} {79};set_instance_parameter_value {router_006} {PKT_DEST_ID_L} {77};set_instance_parameter_value {router_006} {PKT_TRANS_WRITE} {55};set_instance_parameter_value {router_006} {PKT_TRANS_READ} {56};set_instance_parameter_value {router_006} {ST_DATA_W} {93};set_instance_parameter_value {router_006} {ST_CHANNEL_W} {5};set_instance_parameter_value {router_006} {DECODER_TYPE} {1};set_instance_parameter_value {router_006} {DEFAULT_CHANNEL} {0};set_instance_parameter_value {router_006} {DEFAULT_WR_CHANNEL} {-1};set_instance_parameter_value {router_006} {DEFAULT_RD_CHANNEL} {-1};set_instance_parameter_value {router_006} {DEFAULT_DESTID} {0};set_instance_parameter_value {router_006} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {router_006} {MEMORY_ALIASING_DECODE} {0};add_instance {hex7led_0_avalon_slave_0_burst_adapter} {altera_merlin_burst_adapter};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_ADDR_H} {34};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_ADDR_L} {18};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BEGIN_BURST} {54};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BYTE_CNT_H} {43};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BYTE_CNT_L} {41};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BYTEEN_H} {17};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BYTEEN_L} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURST_SIZE_H} {49};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURST_SIZE_L} {47};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURST_TYPE_H} {51};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURST_TYPE_L} {50};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURSTWRAP_H} {46};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_BURSTWRAP_L} {44};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_TRANS_COMPRESSED_READ} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_TRANS_WRITE} {37};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PKT_TRANS_READ} {38};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {OUT_NARROW_SIZE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {IN_NARROW_SIZE} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {OUT_FIXED} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {OUT_COMPLETE_WRAP} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {ST_DATA_W} {75};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {ST_CHANNEL_W} {5};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {OUT_BYTE_CNT_H} {42};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {OUT_BURSTWRAP_H} {46};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {MERLIN_PACKET_FORMAT} {ori_burst_size(74:72) response_status(71:70) cache(69:66) protection(65:63) thread_id(62) dest_id(61:59) src_id(58:56) qos(55) begin_burst(54) data_sideband(53) addr_sideband(52) burst_type(51:50) burst_size(49:47) burstwrap(46:44) byte_cnt(43:41) trans_exclusive(40) trans_lock(39) trans_read(38) trans_write(37) trans_posted(36) trans_compressed_read(35) addr(34:18) byteen(17:16) data(15:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {COMPRESSED_READ_SUPPORT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {BYTEENABLE_SYNTHESIS} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {PIPE_INPUTS} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {NO_WRAP_SUPPORT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {INCOMPLETE_WRAP_SUPPORT} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {BURSTWRAP_CONST_MASK} {7};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {BURSTWRAP_CONST_VALUE} {7};set_instance_parameter_value {hex7led_0_avalon_slave_0_burst_adapter} {ADAPTER_VERSION} {13.1};add_instance {cmd_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux} {ST_DATA_W} {93};set_instance_parameter_value {cmd_demux} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_demux} {NUM_OUTPUTS} {5};set_instance_parameter_value {cmd_demux} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_demux_001} {altera_merlin_demultiplexer};set_instance_parameter_value {cmd_demux_001} {ST_DATA_W} {93};set_instance_parameter_value {cmd_demux_001} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_demux_001} {NUM_OUTPUTS} {2};set_instance_parameter_value {cmd_demux_001} {VALID_WIDTH} {1};set_instance_parameter_value {cmd_demux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_mux} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux} {ST_DATA_W} {93};set_instance_parameter_value {cmd_mux} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_mux} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux} {PIPELINE_ARB} {1};set_instance_parameter_value {cmd_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {cmd_mux} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_mux_001} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_001} {ST_DATA_W} {93};set_instance_parameter_value {cmd_mux_001} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_mux_001} {NUM_INPUTS} {2};set_instance_parameter_value {cmd_mux_001} {PIPELINE_ARB} {1};set_instance_parameter_value {cmd_mux_001} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_001} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {cmd_mux_001} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_001} {ARBITRATION_SHARES} {1 1 };set_instance_parameter_value {cmd_mux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_mux_002} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_002} {ST_DATA_W} {93};set_instance_parameter_value {cmd_mux_002} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_mux_002} {NUM_INPUTS} {2};set_instance_parameter_value {cmd_mux_002} {PIPELINE_ARB} {1};set_instance_parameter_value {cmd_mux_002} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_002} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {cmd_mux_002} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_002} {ARBITRATION_SHARES} {1 1 };set_instance_parameter_value {cmd_mux_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_mux_003} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_003} {ST_DATA_W} {93};set_instance_parameter_value {cmd_mux_003} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_mux_003} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux_003} {PIPELINE_ARB} {1};set_instance_parameter_value {cmd_mux_003} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_003} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {cmd_mux_003} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_003} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux_003} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {cmd_mux_004} {altera_merlin_multiplexer};set_instance_parameter_value {cmd_mux_004} {ST_DATA_W} {93};set_instance_parameter_value {cmd_mux_004} {ST_CHANNEL_W} {5};set_instance_parameter_value {cmd_mux_004} {NUM_INPUTS} {1};set_instance_parameter_value {cmd_mux_004} {PIPELINE_ARB} {1};set_instance_parameter_value {cmd_mux_004} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {cmd_mux_004} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {cmd_mux_004} {ARBITRATION_SCHEME} {round-robin};set_instance_parameter_value {cmd_mux_004} {ARBITRATION_SHARES} {1 };set_instance_parameter_value {cmd_mux_004} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_demux} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux} {ST_DATA_W} {93};set_instance_parameter_value {rsp_demux} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_demux} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_demux_001} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_001} {ST_DATA_W} {93};set_instance_parameter_value {rsp_demux_001} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_demux_001} {NUM_OUTPUTS} {2};set_instance_parameter_value {rsp_demux_001} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_demux_002} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_002} {ST_DATA_W} {93};set_instance_parameter_value {rsp_demux_002} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_demux_002} {NUM_OUTPUTS} {2};set_instance_parameter_value {rsp_demux_002} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_002} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_demux_003} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_003} {ST_DATA_W} {93};set_instance_parameter_value {rsp_demux_003} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_demux_003} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux_003} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_003} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_demux_004} {altera_merlin_demultiplexer};set_instance_parameter_value {rsp_demux_004} {ST_DATA_W} {93};set_instance_parameter_value {rsp_demux_004} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_demux_004} {NUM_OUTPUTS} {1};set_instance_parameter_value {rsp_demux_004} {VALID_WIDTH} {1};set_instance_parameter_value {rsp_demux_004} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_mux} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux} {ST_DATA_W} {93};set_instance_parameter_value {rsp_mux} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_mux} {NUM_INPUTS} {5};set_instance_parameter_value {rsp_mux} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {rsp_mux} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux} {ARBITRATION_SHARES} {1 1 1 1 1 };set_instance_parameter_value {rsp_mux} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {rsp_mux_001} {altera_merlin_multiplexer};set_instance_parameter_value {rsp_mux_001} {ST_DATA_W} {93};set_instance_parameter_value {rsp_mux_001} {ST_CHANNEL_W} {5};set_instance_parameter_value {rsp_mux_001} {NUM_INPUTS} {2};set_instance_parameter_value {rsp_mux_001} {PIPELINE_ARB} {0};set_instance_parameter_value {rsp_mux_001} {USE_EXTERNAL_ARB} {0};set_instance_parameter_value {rsp_mux_001} {PKT_TRANS_LOCK} {57};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SCHEME} {no-arb};set_instance_parameter_value {rsp_mux_001} {ARBITRATION_SHARES} {1 1 };set_instance_parameter_value {rsp_mux_001} {MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};add_instance {hex7led_0_avalon_slave_0_rsp_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_ADDR_H} {34};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_ADDR_L} {18};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_DATA_H} {15};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BYTEEN_H} {17};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BYTEEN_L} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BYTE_CNT_H} {43};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BYTE_CNT_L} {41};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_TRANS_WRITE} {37};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURSTWRAP_H} {46};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURSTWRAP_L} {44};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURST_SIZE_H} {49};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURST_SIZE_L} {47};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {71};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {70};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {40};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURST_TYPE_H} {51};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_BURST_TYPE_L} {50};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {72};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {74};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_ST_DATA_W} {75};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_ADDR_H} {52};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_ADDR_L} {36};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_DATA_H} {31};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BYTEEN_H} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BYTEEN_L} {32};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BYTE_CNT_H} {61};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BYTE_CNT_L} {59};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BURST_SIZE_H} {67};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BURST_SIZE_L} {65};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {58};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BURST_TYPE_H} {69};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_BURST_TYPE_L} {68};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_ST_DATA_W} {93};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {ST_CHANNEL_W} {5};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OPTIMIZE_FOR_RSP} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {RESPONSE_PATH} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {PACKING} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(74:72) response_status(71:70) cache(69:66) protection(65:63) thread_id(62) dest_id(61:59) src_id(58:56) qos(55) begin_burst(54) data_sideband(53) addr_sideband(52) burst_type(51:50) burst_size(49:47) burstwrap(46:44) byte_cnt(43:41) trans_exclusive(40) trans_lock(39) trans_read(38) trans_write(37) trans_posted(36) trans_compressed_read(35) addr(34:18) byteen(17:16) data(15:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {hex7led_0_avalon_slave_0_rsp_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {hex7led_0_avalon_slave_0_cmd_width_adapter} {altera_merlin_width_adapter};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_ADDR_H} {52};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_ADDR_L} {36};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_DATA_H} {31};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_DATA_L} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BYTEEN_H} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BYTEEN_L} {32};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BYTE_CNT_H} {61};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BYTE_CNT_L} {59};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_TRANS_COMPRESSED_READ} {53};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_TRANS_WRITE} {55};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURSTWRAP_H} {64};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURSTWRAP_L} {62};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURST_SIZE_H} {67};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURST_SIZE_L} {65};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_H} {89};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_RESPONSE_STATUS_L} {88};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_TRANS_EXCLUSIVE} {58};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURST_TYPE_H} {69};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_BURST_TYPE_L} {68};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_L} {90};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_PKT_ORI_BURST_SIZE_H} {92};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_ST_DATA_W} {93};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_ADDR_H} {34};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_ADDR_L} {18};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_DATA_H} {15};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_DATA_L} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BYTEEN_H} {17};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BYTEEN_L} {16};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BYTE_CNT_H} {43};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BYTE_CNT_L} {41};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_TRANS_COMPRESSED_READ} {35};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BURST_SIZE_H} {49};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BURST_SIZE_L} {47};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_H} {71};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_RESPONSE_STATUS_L} {70};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_TRANS_EXCLUSIVE} {40};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BURST_TYPE_H} {51};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_BURST_TYPE_L} {50};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_L} {72};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_PKT_ORI_BURST_SIZE_H} {74};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_ST_DATA_W} {75};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {ST_CHANNEL_W} {5};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OPTIMIZE_FOR_RSP} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {RESPONSE_PATH} {0};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {CONSTANT_BURST_SIZE} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {PACKING} {1};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {IN_MERLIN_PACKET_FORMAT} {ori_burst_size(92:90) response_status(89:88) cache(87:84) protection(83:81) thread_id(80) dest_id(79:77) src_id(76:74) qos(73) begin_burst(72) data_sideband(71) addr_sideband(70) burst_type(69:68) burst_size(67:65) burstwrap(64:62) byte_cnt(61:59) trans_exclusive(58) trans_lock(57) trans_read(56) trans_write(55) trans_posted(54) trans_compressed_read(53) addr(52:36) byteen(35:32) data(31:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {OUT_MERLIN_PACKET_FORMAT} {ori_burst_size(74:72) response_status(71:70) cache(69:66) protection(65:63) thread_id(62) dest_id(61:59) src_id(58:56) qos(55) begin_burst(54) data_sideband(53) addr_sideband(52) burst_type(51:50) burst_size(49:47) burstwrap(46:44) byte_cnt(43:41) trans_exclusive(40) trans_lock(39) trans_read(38) trans_write(37) trans_posted(36) trans_compressed_read(35) addr(34:18) byteen(17:16) data(15:0)};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {COMMAND_SIZE_W} {3};set_instance_parameter_value {hex7led_0_avalon_slave_0_cmd_width_adapter} {ENABLE_ADDRESS_ALIGNMENT} {0};add_instance {nios2_gen2_0_reset_reset_bridge} {altera_reset_bridge};set_instance_parameter_value {nios2_gen2_0_reset_reset_bridge} {ACTIVE_LOW_RESET} {0};set_instance_parameter_value {nios2_gen2_0_reset_reset_bridge} {SYNCHRONOUS_EDGES} {deassert};set_instance_parameter_value {nios2_gen2_0_reset_reset_bridge} {NUM_RESET_OUTPUTS} {1};set_instance_parameter_value {nios2_gen2_0_reset_reset_bridge} {USE_RESET_REQUEST} {0};add_instance {clk_0_clk_clock_bridge} {altera_clock_bridge};set_instance_parameter_value {clk_0_clk_clock_bridge} {EXPLICIT_CLOCK_RATE} {20000000};set_instance_parameter_value {clk_0_clk_clock_bridge} {NUM_CLOCK_OUTPUTS} {1};add_connection {nios2_gen2_0_data_master_translator.avalon_universal_master_0} {nios2_gen2_0_data_master_agent.av} {avalon};set_connection_parameter_value {nios2_gen2_0_data_master_translator.avalon_universal_master_0/nios2_gen2_0_data_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {nios2_gen2_0_data_master_translator.avalon_universal_master_0/nios2_gen2_0_data_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {nios2_gen2_0_data_master_translator.avalon_universal_master_0/nios2_gen2_0_data_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux.src} {nios2_gen2_0_data_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux.src/nios2_gen2_0_data_master_agent.rp} {qsys_mm.response};add_connection {nios2_gen2_0_instruction_master_translator.avalon_universal_master_0} {nios2_gen2_0_instruction_master_agent.av} {avalon};set_connection_parameter_value {nios2_gen2_0_instruction_master_translator.avalon_universal_master_0/nios2_gen2_0_instruction_master_agent.av} {arbitrationPriority} {1};set_connection_parameter_value {nios2_gen2_0_instruction_master_translator.avalon_universal_master_0/nios2_gen2_0_instruction_master_agent.av} {baseAddress} {0x0000};set_connection_parameter_value {nios2_gen2_0_instruction_master_translator.avalon_universal_master_0/nios2_gen2_0_instruction_master_agent.av} {defaultConnection} {false};add_connection {rsp_mux_001.src} {nios2_gen2_0_instruction_master_agent.rp} {avalon_streaming};preview_set_connection_tag {rsp_mux_001.src/nios2_gen2_0_instruction_master_agent.rp} {qsys_mm.response};add_connection {hex7led_0_avalon_slave_0_agent.m0} {hex7led_0_avalon_slave_0_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {hex7led_0_avalon_slave_0_agent.m0/hex7led_0_avalon_slave_0_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {hex7led_0_avalon_slave_0_agent.m0/hex7led_0_avalon_slave_0_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {hex7led_0_avalon_slave_0_agent.m0/hex7led_0_avalon_slave_0_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {hex7led_0_avalon_slave_0_agent.rf_source} {hex7led_0_avalon_slave_0_agent_rsp_fifo.in} {avalon_streaming};add_connection {hex7led_0_avalon_slave_0_agent_rsp_fifo.out} {hex7led_0_avalon_slave_0_agent.rf_sink} {avalon_streaming};add_connection {hex7led_0_avalon_slave_0_agent.rdata_fifo_src} {hex7led_0_avalon_slave_0_agent.rdata_fifo_sink} {avalon_streaming};add_connection {nios2_gen2_0_debug_mem_slave_agent.m0} {nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {nios2_gen2_0_debug_mem_slave_agent.m0/nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {nios2_gen2_0_debug_mem_slave_agent.m0/nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {nios2_gen2_0_debug_mem_slave_agent.m0/nios2_gen2_0_debug_mem_slave_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {nios2_gen2_0_debug_mem_slave_agent.rf_source} {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo.in} {avalon_streaming};add_connection {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo.out} {nios2_gen2_0_debug_mem_slave_agent.rf_sink} {avalon_streaming};add_connection {nios2_gen2_0_debug_mem_slave_agent.rdata_fifo_src} {nios2_gen2_0_debug_mem_slave_agent.rdata_fifo_sink} {avalon_streaming};add_connection {cmd_mux_001.src} {nios2_gen2_0_debug_mem_slave_agent.cp} {avalon_streaming};preview_set_connection_tag {cmd_mux_001.src/nios2_gen2_0_debug_mem_slave_agent.cp} {qsys_mm.command};add_connection {onchip_memory2_0_s1_agent.m0} {onchip_memory2_0_s1_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {onchip_memory2_0_s1_agent.m0/onchip_memory2_0_s1_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {onchip_memory2_0_s1_agent.rf_source} {onchip_memory2_0_s1_agent_rsp_fifo.in} {avalon_streaming};add_connection {onchip_memory2_0_s1_agent_rsp_fifo.out} {onchip_memory2_0_s1_agent.rf_sink} {avalon_streaming};add_connection {onchip_memory2_0_s1_agent.rdata_fifo_src} {onchip_memory2_0_s1_agent.rdata_fifo_sink} {avalon_streaming};add_connection {cmd_mux_002.src} {onchip_memory2_0_s1_agent.cp} {avalon_streaming};preview_set_connection_tag {cmd_mux_002.src/onchip_memory2_0_s1_agent.cp} {qsys_mm.command};add_connection {timer_0_s1_agent.m0} {timer_0_s1_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {timer_0_s1_agent.m0/timer_0_s1_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {timer_0_s1_agent.m0/timer_0_s1_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {timer_0_s1_agent.m0/timer_0_s1_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {timer_0_s1_agent.rf_source} {timer_0_s1_agent_rsp_fifo.in} {avalon_streaming};add_connection {timer_0_s1_agent_rsp_fifo.out} {timer_0_s1_agent.rf_sink} {avalon_streaming};add_connection {timer_0_s1_agent.rdata_fifo_src} {timer_0_s1_agent.rdata_fifo_sink} {avalon_streaming};add_connection {cmd_mux_003.src} {timer_0_s1_agent.cp} {avalon_streaming};preview_set_connection_tag {cmd_mux_003.src/timer_0_s1_agent.cp} {qsys_mm.command};add_connection {pio_0_s1_agent.m0} {pio_0_s1_translator.avalon_universal_slave_0} {avalon};set_connection_parameter_value {pio_0_s1_agent.m0/pio_0_s1_translator.avalon_universal_slave_0} {arbitrationPriority} {1};set_connection_parameter_value {pio_0_s1_agent.m0/pio_0_s1_translator.avalon_universal_slave_0} {baseAddress} {0x0000};set_connection_parameter_value {pio_0_s1_agent.m0/pio_0_s1_translator.avalon_universal_slave_0} {defaultConnection} {false};add_connection {pio_0_s1_agent.rf_source} {pio_0_s1_agent_rsp_fifo.in} {avalon_streaming};add_connection {pio_0_s1_agent_rsp_fifo.out} {pio_0_s1_agent.rf_sink} {avalon_streaming};add_connection {pio_0_s1_agent.rdata_fifo_src} {pio_0_s1_agent.rdata_fifo_sink} {avalon_streaming};add_connection {cmd_mux_004.src} {pio_0_s1_agent.cp} {avalon_streaming};preview_set_connection_tag {cmd_mux_004.src/pio_0_s1_agent.cp} {qsys_mm.command};add_connection {nios2_gen2_0_data_master_agent.cp} {router.sink} {avalon_streaming};preview_set_connection_tag {nios2_gen2_0_data_master_agent.cp/router.sink} {qsys_mm.command};add_connection {router.src} {cmd_demux.sink} {avalon_streaming};preview_set_connection_tag {router.src/cmd_demux.sink} {qsys_mm.command};add_connection {nios2_gen2_0_instruction_master_agent.cp} {router_001.sink} {avalon_streaming};preview_set_connection_tag {nios2_gen2_0_instruction_master_agent.cp/router_001.sink} {qsys_mm.command};add_connection {router_001.src} {cmd_demux_001.sink} {avalon_streaming};preview_set_connection_tag {router_001.src/cmd_demux_001.sink} {qsys_mm.command};add_connection {hex7led_0_avalon_slave_0_agent.rp} {router_002.sink} {avalon_streaming};preview_set_connection_tag {hex7led_0_avalon_slave_0_agent.rp/router_002.sink} {qsys_mm.response};add_connection {nios2_gen2_0_debug_mem_slave_agent.rp} {router_003.sink} {avalon_streaming};preview_set_connection_tag {nios2_gen2_0_debug_mem_slave_agent.rp/router_003.sink} {qsys_mm.response};add_connection {router_003.src} {rsp_demux_001.sink} {avalon_streaming};preview_set_connection_tag {router_003.src/rsp_demux_001.sink} {qsys_mm.response};add_connection {onchip_memory2_0_s1_agent.rp} {router_004.sink} {avalon_streaming};preview_set_connection_tag {onchip_memory2_0_s1_agent.rp/router_004.sink} {qsys_mm.response};add_connection {router_004.src} {rsp_demux_002.sink} {avalon_streaming};preview_set_connection_tag {router_004.src/rsp_demux_002.sink} {qsys_mm.response};add_connection {timer_0_s1_agent.rp} {router_005.sink} {avalon_streaming};preview_set_connection_tag {timer_0_s1_agent.rp/router_005.sink} {qsys_mm.response};add_connection {router_005.src} {rsp_demux_003.sink} {avalon_streaming};preview_set_connection_tag {router_005.src/rsp_demux_003.sink} {qsys_mm.response};add_connection {pio_0_s1_agent.rp} {router_006.sink} {avalon_streaming};preview_set_connection_tag {pio_0_s1_agent.rp/router_006.sink} {qsys_mm.response};add_connection {router_006.src} {rsp_demux_004.sink} {avalon_streaming};preview_set_connection_tag {router_006.src/rsp_demux_004.sink} {qsys_mm.response};add_connection {hex7led_0_avalon_slave_0_burst_adapter.source0} {hex7led_0_avalon_slave_0_agent.cp} {avalon_streaming};preview_set_connection_tag {hex7led_0_avalon_slave_0_burst_adapter.source0/hex7led_0_avalon_slave_0_agent.cp} {qsys_mm.command};add_connection {cmd_demux.src0} {cmd_mux.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src0/cmd_mux.sink0} {qsys_mm.command};add_connection {cmd_demux.src1} {cmd_mux_001.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src1/cmd_mux_001.sink0} {qsys_mm.command};add_connection {cmd_demux.src2} {cmd_mux_002.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src2/cmd_mux_002.sink0} {qsys_mm.command};add_connection {cmd_demux.src3} {cmd_mux_003.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src3/cmd_mux_003.sink0} {qsys_mm.command};add_connection {cmd_demux.src4} {cmd_mux_004.sink0} {avalon_streaming};preview_set_connection_tag {cmd_demux.src4/cmd_mux_004.sink0} {qsys_mm.command};add_connection {cmd_demux_001.src0} {cmd_mux_001.sink1} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src0/cmd_mux_001.sink1} {qsys_mm.command};add_connection {cmd_demux_001.src1} {cmd_mux_002.sink1} {avalon_streaming};preview_set_connection_tag {cmd_demux_001.src1/cmd_mux_002.sink1} {qsys_mm.command};add_connection {rsp_demux.src0} {rsp_mux.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux.src0/rsp_mux.sink0} {qsys_mm.response};add_connection {rsp_demux_001.src0} {rsp_mux.sink1} {avalon_streaming};preview_set_connection_tag {rsp_demux_001.src0/rsp_mux.sink1} {qsys_mm.response};add_connection {rsp_demux_001.src1} {rsp_mux_001.sink0} {avalon_streaming};preview_set_connection_tag {rsp_demux_001.src1/rsp_mux_001.sink0} {qsys_mm.response};add_connection {rsp_demux_002.src0} {rsp_mux.sink2} {avalon_streaming};preview_set_connection_tag {rsp_demux_002.src0/rsp_mux.sink2} {qsys_mm.response};add_connection {rsp_demux_002.src1} {rsp_mux_001.sink1} {avalon_streaming};preview_set_connection_tag {rsp_demux_002.src1/rsp_mux_001.sink1} {qsys_mm.response};add_connection {rsp_demux_003.src0} {rsp_mux.sink3} {avalon_streaming};preview_set_connection_tag {rsp_demux_003.src0/rsp_mux.sink3} {qsys_mm.response};add_connection {rsp_demux_004.src0} {rsp_mux.sink4} {avalon_streaming};preview_set_connection_tag {rsp_demux_004.src0/rsp_mux.sink4} {qsys_mm.response};add_connection {router_002.src} {hex7led_0_avalon_slave_0_rsp_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {router_002.src/hex7led_0_avalon_slave_0_rsp_width_adapter.sink} {qsys_mm.response};add_connection {hex7led_0_avalon_slave_0_rsp_width_adapter.src} {rsp_demux.sink} {avalon_streaming};preview_set_connection_tag {hex7led_0_avalon_slave_0_rsp_width_adapter.src/rsp_demux.sink} {qsys_mm.response};add_connection {cmd_mux.src} {hex7led_0_avalon_slave_0_cmd_width_adapter.sink} {avalon_streaming};preview_set_connection_tag {cmd_mux.src/hex7led_0_avalon_slave_0_cmd_width_adapter.sink} {qsys_mm.command};add_connection {hex7led_0_avalon_slave_0_cmd_width_adapter.src} {hex7led_0_avalon_slave_0_burst_adapter.sink0} {avalon_streaming};preview_set_connection_tag {hex7led_0_avalon_slave_0_cmd_width_adapter.src/hex7led_0_avalon_slave_0_burst_adapter.sink0} {qsys_mm.command};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_data_master_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_instruction_master_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_debug_mem_slave_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {onchip_memory2_0_s1_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {timer_0_s1_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {pio_0_s1_translator.reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_data_master_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_instruction_master_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_agent_rsp_fifo.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_debug_mem_slave_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {onchip_memory2_0_s1_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {onchip_memory2_0_s1_agent_rsp_fifo.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {timer_0_s1_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {timer_0_s1_agent_rsp_fifo.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {pio_0_s1_agent.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {pio_0_s1_agent_rsp_fifo.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_001.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_002.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_003.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_004.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_005.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {router_006.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_burst_adapter.cr0_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_demux.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_demux_001.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_mux.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_mux_001.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_mux_002.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_mux_003.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {cmd_mux_004.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_demux.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_demux_001.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_demux_002.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_demux_003.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_demux_004.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_mux.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {rsp_mux_001.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_rsp_width_adapter.clk_reset} {reset};add_connection {nios2_gen2_0_reset_reset_bridge.out_reset} {hex7led_0_avalon_slave_0_cmd_width_adapter.clk_reset} {reset};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_data_master_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_instruction_master_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_debug_mem_slave_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {onchip_memory2_0_s1_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {timer_0_s1_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {pio_0_s1_translator.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_data_master_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_instruction_master_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_agent_rsp_fifo.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_debug_mem_slave_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_debug_mem_slave_agent_rsp_fifo.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {onchip_memory2_0_s1_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {onchip_memory2_0_s1_agent_rsp_fifo.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {timer_0_s1_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {timer_0_s1_agent_rsp_fifo.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {pio_0_s1_agent.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {pio_0_s1_agent_rsp_fifo.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_001.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_002.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_003.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_004.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_005.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {router_006.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_burst_adapter.cr0} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_demux.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_mux.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_demux_001.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_mux_001.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_mux.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_demux.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_mux_001.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_demux_001.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_mux_002.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_demux_002.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_mux_003.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_demux_003.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {cmd_mux_004.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {rsp_demux_004.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_rsp_width_adapter.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {hex7led_0_avalon_slave_0_cmd_width_adapter.clk} {clock};add_connection {clk_0_clk_clock_bridge.out_clk} {nios2_gen2_0_reset_reset_bridge.clk} {clock};add_interface {clk_0_clk} {clock} {slave};set_interface_property {clk_0_clk} {EXPORT_OF} {clk_0_clk_clock_bridge.in_clk};add_interface {nios2_gen2_0_reset_reset_bridge_in_reset} {reset} {slave};set_interface_property {nios2_gen2_0_reset_reset_bridge_in_reset} {EXPORT_OF} {nios2_gen2_0_reset_reset_bridge.in_reset};add_interface {nios2_gen2_0_data_master} {avalon} {slave};set_interface_property {nios2_gen2_0_data_master} {EXPORT_OF} {nios2_gen2_0_data_master_translator.avalon_anti_master_0};add_interface {nios2_gen2_0_instruction_master} {avalon} {slave};set_interface_property {nios2_gen2_0_instruction_master} {EXPORT_OF} {nios2_gen2_0_instruction_master_translator.avalon_anti_master_0};add_interface {hex7led_0_avalon_slave_0} {avalon} {master};set_interface_property {hex7led_0_avalon_slave_0} {EXPORT_OF} {hex7led_0_avalon_slave_0_translator.avalon_anti_slave_0};add_interface {nios2_gen2_0_debug_mem_slave} {avalon} {master};set_interface_property {nios2_gen2_0_debug_mem_slave} {EXPORT_OF} {nios2_gen2_0_debug_mem_slave_translator.avalon_anti_slave_0};add_interface {onchip_memory2_0_s1} {avalon} {master};set_interface_property {onchip_memory2_0_s1} {EXPORT_OF} {onchip_memory2_0_s1_translator.avalon_anti_slave_0};add_interface {pio_0_s1} {avalon} {master};set_interface_property {pio_0_s1} {EXPORT_OF} {pio_0_s1_translator.avalon_anti_slave_0};add_interface {timer_0_s1} {avalon} {master};set_interface_property {timer_0_s1} {EXPORT_OF} {timer_0_s1_translator.avalon_anti_slave_0};set_module_assignment {interconnect_id.hex7led_0.avalon_slave_0} {0};set_module_assignment {interconnect_id.nios2_gen2_0.data_master} {0};set_module_assignment {interconnect_id.nios2_gen2_0.debug_mem_slave} {1};set_module_assignment {interconnect_id.nios2_gen2_0.instruction_master} {1};set_module_assignment {interconnect_id.onchip_memory2_0.s1} {2};set_module_assignment {interconnect_id.pio_0.s1} {3};set_module_assignment {interconnect_id.timer_0.s1} {4};]]></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>MAX10FPGA</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE">
   <type>java.lang.String</type>
   <value>10M08DAF256C8GES</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE</sysinfo_type>
  </parameter>
  <parameter name="AUTO_DEVICE_SPEEDGRADE">
   <type>java.lang.String</type>
   <value></value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_SPEEDGRADE</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>MAX 10</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk_0_clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk_0_clk_clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface
     name="nios2_gen2_0_reset_reset_bridge_in_reset"
     kind="reset_sink"
     version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>nios2_gen2_0_reset_reset_bridge_in_reset_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="nios2_gen2_0_data_master" kind="avalon_slave" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>131072</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>nios2_gen2_0_data_master_address</name>
    <direction>Input</direction>
    <width>17</width>
    <role>address</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_byteenable</name>
    <direction>Input</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_write</name>
    <direction>Input</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_writedata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>nios2_gen2_0_data_master_debugaccess</name>
    <direction>Input</direction>
    <width>1</width>
    <role>debugaccess</role>
   </port>
  </interface>
  <interface
     name="nios2_gen2_0_instruction_master"
     kind="avalon_slave"
     version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <assignment>
    <name>embeddedsw.configuration.isFlash</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isMemoryDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isNonVolatileStorage</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>embeddedsw.configuration.isPrintableDevice</name>
    <value>0</value>
   </assignment>
   <assignment>
    <name>merlin.flow.avalon_universal_master_0</name>
    <value>avalon_universal_master_0</value>
   </assignment>
   <parameter name="addressAlignment">
    <type>com.altera.sopcmodel.avalon.AvalonConnectionPoint$AddressAlignment</type>
    <value>DYNAMIC</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressSpan">
    <type>java.math.BigInteger</type>
    <value>131072</value>
    <derived>true</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>SYMBOLS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedAddressOffset">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToMaster">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="explicitAddressSpan">
    <type>java.math.BigInteger</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isFlash">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isMemoryDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isNonVolatileStorage">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>false</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="minimumUninterruptedRunLength">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="printableDevice">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitStates">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="transparentBridge">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="wellBehavedWaitrequest">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitStates">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>false</isStart>
   <port>
    <name>nios2_gen2_0_instruction_master_address</name>
    <direction>Input</direction>
    <width>17</width>
    <role>address</role>
   </port>
   <port>
    <name>nios2_gen2_0_instruction_master_waitrequest</name>
    <direction>Output</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>nios2_gen2_0_instruction_master_read</name>
    <direction>Input</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>nios2_gen2_0_instruction_master_readdata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
  </interface>
  <interface name="hex7led_0_avalon_slave_0" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>hex7led_0_avalon_slave_0_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>hex7led_0_avalon_slave_0_writedata</name>
    <direction>Output</direction>
    <width>16</width>
    <role>writedata</role>
   </port>
   <port>
    <name>hex7led_0_avalon_slave_0_byteenable</name>
    <direction>Output</direction>
    <width>2</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>hex7led_0_avalon_slave_0_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>hex7led_0</moduleName>
    <slaveName>avalon_slave_0</slaveName>
    <name>hex7led_0.avalon_slave_0</name>
    <baseAddress>0</baseAddress>
    <span>2</span>
   </memoryBlock>
  </interface>
  <interface
     name="nios2_gen2_0_debug_mem_slave"
     kind="avalon_master"
     version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>true</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_address</name>
    <direction>Output</direction>
    <width>9</width>
    <role>address</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_read</name>
    <direction>Output</direction>
    <width>1</width>
    <role>read</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_byteenable</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_waitrequest</name>
    <direction>Input</direction>
    <width>1</width>
    <role>waitrequest</role>
   </port>
   <port>
    <name>nios2_gen2_0_debug_mem_slave_debugaccess</name>
    <direction>Output</direction>
    <width>1</width>
    <role>debugaccess</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>nios2_gen2_0</moduleName>
    <slaveName>debug_mem_slave</slaveName>
    <name>nios2_gen2_0.debug_mem_slave</name>
    <baseAddress>0</baseAddress>
    <span>2048</span>
   </memoryBlock>
  </interface>
  <interface name="onchip_memory2_0_s1" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>onchip_memory2_0_s1_address</name>
    <direction>Output</direction>
    <width>13</width>
    <role>address</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_byteenable</name>
    <direction>Output</direction>
    <width>4</width>
    <role>byteenable</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <port>
    <name>onchip_memory2_0_s1_clken</name>
    <direction>Output</direction>
    <width>1</width>
    <role>clken</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>onchip_memory2_0</moduleName>
    <slaveName>s1</slaveName>
    <name>onchip_memory2_0.s1</name>
    <baseAddress>0</baseAddress>
    <span>32768</span>
   </memoryBlock>
  </interface>
  <interface name="pio_0_s1" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>pio_0_s1_address</name>
    <direction>Output</direction>
    <width>2</width>
    <role>address</role>
   </port>
   <port>
    <name>pio_0_s1_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>pio_0_s1_readdata</name>
    <direction>Input</direction>
    <width>32</width>
    <role>readdata</role>
   </port>
   <port>
    <name>pio_0_s1_writedata</name>
    <direction>Output</direction>
    <width>32</width>
    <role>writedata</role>
   </port>
   <port>
    <name>pio_0_s1_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>pio_0</moduleName>
    <slaveName>s1</slaveName>
    <name>pio_0.s1</name>
    <baseAddress>0</baseAddress>
    <span>16</span>
   </memoryBlock>
  </interface>
  <interface name="timer_0_s1" kind="avalon_master" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="adaptsTo">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressGroup">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="addressUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="alwaysBurstMaxBurst">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk_0_clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>nios2_gen2_0_reset_reset_bridge_in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bitsPerSymbol">
    <type>int</type>
    <value>8</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstOnBurstBoundariesOnly">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="burstcountUnits">
    <type>com.altera.sopcmodel.avalon.EAddrBurstUnits</type>
    <value>WORDS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="constantBurstBehavior">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="dBSBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamReads">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="doStreamWrites">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="holdTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="interleaveBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isAsynchronous">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isBigEndian">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isReadable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="isWriteable">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="linewrapBursts">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maxAddressWidth">
    <type>int</type>
    <value>32</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingReadTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="maximumPendingWriteTransactions">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readLatency">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="readWaitTime">
    <type>int</type>
    <value>1</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerIncomingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="registerOutgoingSignals">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="setupTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="timingUnits">
    <type>com.altera.sopcmodel.avalon.TimingUnits</type>
    <value>Cycles</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="writeWaitTime">
    <type>int</type>
    <value>0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>avalon</type>
   <isStart>true</isStart>
   <port>
    <name>timer_0_s1_address</name>
    <direction>Output</direction>
    <width>3</width>
    <role>address</role>
   </port>
   <port>
    <name>timer_0_s1_write</name>
    <direction>Output</direction>
    <width>1</width>
    <role>write</role>
   </port>
   <port>
    <name>timer_0_s1_readdata</name>
    <direction>Input</direction>
    <width>16</width>
    <role>readdata</role>
   </port>
   <port>
    <name>timer_0_s1_writedata</name>
    <direction>Output</direction>
    <width>16</width>
    <role>writedata</role>
   </port>
   <port>
    <name>timer_0_s1_chipselect</name>
    <direction>Output</direction>
    <width>1</width>
    <role>chipselect</role>
   </port>
   <memoryBlock>
    <isBridge>false</isBridge>
    <moduleName>timer_0</moduleName>
    <slaveName>s1</slaveName>
    <name>timer_0.s1</name>
    <baseAddress>0</baseAddress>
    <span>32</span>
   </memoryBlock>
  </interface>
 </module>
 <module
   name="irq_mapper"
   kind="altera_irq_mapper"
   version="16.0"
   path="irq_mapper">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="NUM_RCVRS">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SENDER_IRQ_WIDTH">
   <type>int</type>
   <value>32</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="IRQ_MAP">
   <type>java.lang.String</type>
   <value>0:0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="AUTO_DEVICE_FAMILY">
   <type>java.lang.String</type>
   <value>MAX10FPGA</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>MAX 10</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
   <sysinfo_type>DEVICE_FAMILY</sysinfo_type>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="clk_reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="receiver0" kind="interrupt_receiver" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedAddressablePoint">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>clk_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqMap">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqScheme">
    <type>com.altera.sopcmodel.interrupt.InterruptConnectionPoint$EIrqScheme</type>
    <value>INDIVIDUAL_REQUESTS</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>interrupt</type>
   <isStart>true</isStart>
   <port>
    <name>receiver0_irq</name>
    <direction>Input</direction>
    <width>1</width>
    <role>irq</role>
   </port>
   <interrupt>
    <isBridge>false</isBridge>
    <moduleName>timer_0</moduleName>
    <slaveName>irq</slaveName>
    <name>timer_0.irq</name>
    <interruptNumber>0</interruptNumber>
   </interrupt>
  </interface>
  <interface name="sender" kind="interrupt_sender" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedAddressablePoint">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedReset">
    <type>java.lang.String</type>
    <value>clk_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgedReceiverOffset">
    <type>java.lang.Integer</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="bridgesToReceiver">
    <type>com.altera.entityinterfaces.IConnectionPoint</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="irqScheme">
    <type>com.altera.sopcmodel.interrupt.InterruptConnectionPoint$EIrqScheme</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>interrupt</type>
   <isStart>false</isStart>
   <port>
    <name>sender_irq</name>
    <direction>Output</direction>
    <width>32</width>
    <role>irq</role>
   </port>
  </interface>
 </module>
 <module
   name="rst_controller"
   kind="altera_reset_controller"
   version="16.0"
   path="rst_controller">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="NUM_RESET_INPUTS">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="OUTPUT_RESET_SYNC_EDGES">
   <type>java.lang.String</type>
   <value>deassert</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SYNC_DEPTH">
   <type>int</type>
   <value>2</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQUEST_PRESENT">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_WAIT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="MIN_RST_ASSERTION_TIME">
   <type>int</type>
   <value>3</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQ_EARLY_DSRT_TIME">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN0">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN1">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN2">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN3">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN4">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN5">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN6">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN7">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN8">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN9">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN10">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN11">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN12">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN13">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN14">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_IN15">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="USE_RESET_REQUEST_INPUT">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="ADAPT_RESET_REQUEST">
   <type>int</type>
   <value>0</value>
   <derived>true</derived>
   <enabled>true</enabled>
   <visible>false</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="reset_in0" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>NONE</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>reset_in0</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="reset_out" kind="reset_source" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>reset_in0</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>reset_out</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
 </module>
 <module
   name="rst_translator"
   kind="altera_reset_translator"
   version="16.0"
   path="rst_translator">
  <!-- Describes a single module. Module parameters are
the requested settings for a module instance. -->
  <parameter name="ACTIVE_LOW_RESET">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="SYNCHRONOUS_EDGES">
   <type>java.lang.String</type>
   <value>deassert</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="RESET_REQUEST_INPUT_ENABLE">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <interface name="clk" kind="clock_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="externallyDriven">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="ptfSchematicName">
    <type>java.lang.String</type>
    <value></value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>false</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>clock</type>
   <isStart>false</isStart>
   <port>
    <name>clk</name>
    <direction>Input</direction>
    <width>1</width>
    <role>clk</role>
   </port>
  </interface>
  <interface name="in_reset" kind="reset_sink" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>false</isStart>
   <port>
    <name>in_reset</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset</role>
   </port>
   <port>
    <name>reset_req_in</name>
    <direction>Input</direction>
    <width>1</width>
    <role>reset_req</role>
   </port>
  </interface>
  <interface name="out_reset" kind="reset_source" version="16.0">
   <!-- The connection points exposed by a module instance for the
particular module parameters. Connection points and their
parameters are a RESULT of the module parameters. -->
   <parameter name="associatedClock">
    <type>java.lang.String</type>
    <value>clk</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedDirectReset">
    <type>java.lang.String</type>
    <value>in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="associatedResetSinks">
    <type>[Ljava.lang.String;</type>
    <value>in_reset</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="synchronousEdges">
    <type>com.altera.sopcmodel.reset.Reset$Edges</type>
    <value>DEASSERT</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="deviceFamily">
    <type>java.lang.String</type>
    <value>UNKNOWN</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <parameter name="generateLegacySim">
    <type>boolean</type>
    <value>false</value>
    <derived>false</derived>
    <enabled>true</enabled>
    <visible>true</visible>
    <valid>true</valid>
   </parameter>
   <type>reset</type>
   <isStart>true</isStart>
   <port>
    <name>out_reset</name>
    <direction>Output</direction>
    <width>1</width>
    <role>reset</role>
   </port>
  </interface>
 </module>
 <connection
   name="clk_0.clk/nios2_gen2_0.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="nios2_gen2_0.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>nios2_gen2_0</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/timer_0.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="timer_0.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>timer_0</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/pio_0.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="pio_0.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>pio_0</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/onchip_memory2_0.clk1"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="onchip_memory2_0.clk1">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>clk1</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/hex7led_0.clock"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="hex7led_0.clock">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>hex7led_0</endModule>
  <endConnectionPoint>clock</endConnectionPoint>
 </connection>
 <connection
   name="nios2_gen2_0.debug_reset_request/clk_0.clk_in_reset"
   kind="reset"
   version="16.0"
   start="nios2_gen2_0.debug_reset_request"
   end="clk_0.clk_in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>nios2_gen2_0</startModule>
  <startConnectionPoint>debug_reset_request</startConnectionPoint>
  <endModule>clk_0</endModule>
  <endConnectionPoint>clk_in_reset</endConnectionPoint>
 </connection>
 <connection
   name="nios2_gen2_0.data_master/mm_interconnect_0.nios2_gen2_0_data_master"
   kind="avalon"
   version="16.0"
   start="nios2_gen2_0.data_master"
   end="mm_interconnect_0.nios2_gen2_0_data_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>nios2_gen2_0</startModule>
  <startConnectionPoint>data_master</startConnectionPoint>
  <endModule>mm_interconnect_0</endModule>
  <endConnectionPoint>nios2_gen2_0_data_master</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/mm_interconnect_0.clk_0_clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="mm_interconnect_0.clk_0_clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>mm_interconnect_0</endModule>
  <endConnectionPoint>clk_0_clk</endConnectionPoint>
 </connection>
 <connection
   name="nios2_gen2_0.instruction_master/mm_interconnect_0.nios2_gen2_0_instruction_master"
   kind="avalon"
   version="16.0"
   start="nios2_gen2_0.instruction_master"
   end="mm_interconnect_0.nios2_gen2_0_instruction_master">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>nios2_gen2_0</startModule>
  <startConnectionPoint>instruction_master</startConnectionPoint>
  <endModule>mm_interconnect_0</endModule>
  <endConnectionPoint>nios2_gen2_0_instruction_master</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_0.hex7led_0_avalon_slave_0/hex7led_0.avalon_slave_0"
   kind="avalon"
   version="16.0"
   start="mm_interconnect_0.hex7led_0_avalon_slave_0"
   end="hex7led_0.avalon_slave_0">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_0</startModule>
  <startConnectionPoint>hex7led_0_avalon_slave_0</startConnectionPoint>
  <endModule>hex7led_0</endModule>
  <endConnectionPoint>avalon_slave_0</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_0.nios2_gen2_0_debug_mem_slave/nios2_gen2_0.debug_mem_slave"
   kind="avalon"
   version="16.0"
   start="mm_interconnect_0.nios2_gen2_0_debug_mem_slave"
   end="nios2_gen2_0.debug_mem_slave">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_0</startModule>
  <startConnectionPoint>nios2_gen2_0_debug_mem_slave</startConnectionPoint>
  <endModule>nios2_gen2_0</endModule>
  <endConnectionPoint>debug_mem_slave</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_0.onchip_memory2_0_s1/onchip_memory2_0.s1"
   kind="avalon"
   version="16.0"
   start="mm_interconnect_0.onchip_memory2_0_s1"
   end="onchip_memory2_0.s1">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_0</startModule>
  <startConnectionPoint>onchip_memory2_0_s1</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>s1</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_0.timer_0_s1/timer_0.s1"
   kind="avalon"
   version="16.0"
   start="mm_interconnect_0.timer_0_s1"
   end="timer_0.s1">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_0</startModule>
  <startConnectionPoint>timer_0_s1</startConnectionPoint>
  <endModule>timer_0</endModule>
  <endConnectionPoint>s1</endConnectionPoint>
 </connection>
 <connection
   name="mm_interconnect_0.pio_0_s1/pio_0.s1"
   kind="avalon"
   version="16.0"
   start="mm_interconnect_0.pio_0_s1"
   end="pio_0.s1">
  <parameter name="arbitrationPriority">
   <type>int</type>
   <value>1</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="baseAddress">
   <type>java.math.BigInteger</type>
   <value>0x0000</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="defaultConnection">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>mm_interconnect_0</startModule>
  <startConnectionPoint>pio_0_s1</startConnectionPoint>
  <endModule>pio_0</endModule>
  <endConnectionPoint>s1</endConnectionPoint>
 </connection>
 <connection
   name="irq_mapper.receiver0/timer_0.irq"
   kind="interrupt"
   version="16.0"
   start="irq_mapper.receiver0"
   end="timer_0.irq">
  <parameter name="irqNumber">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>irq_mapper</startModule>
  <startConnectionPoint>receiver0</startConnectionPoint>
  <endModule>timer_0</endModule>
  <endConnectionPoint>irq</endConnectionPoint>
 </connection>
 <connection
   name="nios2_gen2_0.irq/irq_mapper.sender"
   kind="interrupt"
   version="16.0"
   start="nios2_gen2_0.irq"
   end="irq_mapper.sender">
  <parameter name="irqNumber">
   <type>int</type>
   <value>0</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>nios2_gen2_0</startModule>
  <startConnectionPoint>irq</startConnectionPoint>
  <endModule>irq_mapper</endModule>
  <endConnectionPoint>sender</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/irq_mapper.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="irq_mapper.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>irq_mapper</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/rst_translator.in_reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/hex7led_0.reset"
   kind="reset"
   version="16.0"
   start="rst_translator.out_reset"
   end="hex7led_0.reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>hex7led_0</endModule>
  <endConnectionPoint>reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/nios2_gen2_0.reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="nios2_gen2_0.reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>nios2_gen2_0</endModule>
  <endConnectionPoint>reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/onchip_memory2_0.reset1"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="onchip_memory2_0.reset1">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>onchip_memory2_0</endModule>
  <endConnectionPoint>reset1</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/rst_translator.in_reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/pio_0.reset"
   kind="reset"
   version="16.0"
   start="rst_translator.out_reset"
   end="pio_0.reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>pio_0</endModule>
  <endConnectionPoint>reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/rst_translator.in_reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/timer_0.reset"
   kind="reset"
   version="16.0"
   start="rst_translator.out_reset"
   end="timer_0.reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>timer_0</endModule>
  <endConnectionPoint>reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/rst_translator.in_reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/mm_interconnect_0.nios2_gen2_0_reset_reset_bridge_in_reset"
   kind="reset"
   version="16.0"
   start="rst_translator.out_reset"
   end="mm_interconnect_0.nios2_gen2_0_reset_reset_bridge_in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>mm_interconnect_0</endModule>
  <endConnectionPoint>nios2_gen2_0_reset_reset_bridge_in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_controller.reset_out/rst_translator.in_reset"
   kind="reset"
   version="16.0"
   start="rst_controller.reset_out"
   end="rst_translator.in_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_controller</startModule>
  <startConnectionPoint>reset_out</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>in_reset</endConnectionPoint>
 </connection>
 <connection
   name="rst_translator.out_reset/irq_mapper.clk_reset"
   kind="reset"
   version="16.0"
   start="rst_translator.out_reset"
   end="irq_mapper.clk_reset">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>rst_translator</startModule>
  <startConnectionPoint>out_reset</startConnectionPoint>
  <endModule>irq_mapper</endModule>
  <endConnectionPoint>clk_reset</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk_reset/rst_controller.reset_in0"
   kind="reset"
   version="16.0"
   start="clk_0.clk_reset"
   end="rst_controller.reset_in0">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk_reset</startConnectionPoint>
  <endModule>rst_controller</endModule>
  <endConnectionPoint>reset_in0</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/rst_controller.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="rst_controller.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>rst_controller</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <connection
   name="clk_0.clk/rst_translator.clk"
   kind="clock"
   version="16.0"
   start="clk_0.clk"
   end="rst_translator.clk">
  <parameter name="deviceFamily">
   <type>java.lang.String</type>
   <value>UNKNOWN</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <parameter name="generateLegacySim">
   <type>boolean</type>
   <value>false</value>
   <derived>false</derived>
   <enabled>true</enabled>
   <visible>true</visible>
   <valid>true</valid>
  </parameter>
  <startModule>clk_0</startModule>
  <startConnectionPoint>clk</startConnectionPoint>
  <endModule>rst_translator</endModule>
  <endConnectionPoint>clk</endConnectionPoint>
 </connection>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Clock Source</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Input</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>reset_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Input</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>clock_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Output</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>reset_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Output</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>hex7led</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>hex7led</displayName>
  <version>1.0</version>
 </plugin>
 <plugin>
  <instanceCount>7</instanceCount>
  <name>avalon_slave</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Avalon Memory Mapped Slave</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>9</instanceCount>
  <name>clock_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Clock Input</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>9</instanceCount>
  <name>reset_sink</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Input</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>3</instanceCount>
  <name>conduit_end</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Conduit</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_nios2_gen2</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Nios II Processor</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>7</instanceCount>
  <name>avalon_master</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Avalon Memory Mapped Master</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>2</instanceCount>
  <name>interrupt_receiver</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Interrupt Receiver</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>3</instanceCount>
  <name>reset_source</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Reset Output</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>nios_custom_instruction_master</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Custom Instruction Master</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_avalon_onchip_memory2</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>On-Chip Memory (RAM or ROM)</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_avalon_pio</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>PIO (Parallel I/O)</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_avalon_timer</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Interval Timer</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>2</instanceCount>
  <name>interrupt_sender</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IMutableConnectionPoint</subtype>
  <displayName>Interrupt Sender</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_mm_interconnect</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>MM Interconnect</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_irq_mapper</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Merlin IRQ Mapper</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_reset_controller</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Merlin Reset Controller</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>altera_reset_translator</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IModule</subtype>
  <displayName>Reset Translator</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>5</instanceCount>
  <name>clock</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Clock Connection</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>1</instanceCount>
  <name>reset</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Reset Connection</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>7</instanceCount>
  <name>avalon</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Avalon Memory Mapped Connection</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>4</instanceCount>
  <name>clock</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Clock Connection</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>2</instanceCount>
  <name>interrupt</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Interrupt Connection</displayName>
  <version>16.0</version>
 </plugin>
 <plugin>
  <instanceCount>13</instanceCount>
  <name>reset</name>
  <type>com.altera.entityinterfaces.IElementClass</type>
  <subtype>com.altera.entityinterfaces.IConnection</subtype>
  <displayName>Reset Connection</displayName>
  <version>16.0</version>
 </plugin>
 <reportVersion>16.0 211</reportVersion>
 <uniqueIdentifier>00000000000000E00000015CEA9F0727</uniqueIdentifier>
</EnsembleReport>
