	component NIOS_LED is
		port (
			clk_clk                      : in  std_logic                    := 'X'; -- clk
			hex7led_0_digit_new_signal   : out std_logic_vector(3 downto 0);        -- new_signal
			hex7led_0_segment_new_signal : out std_logic_vector(7 downto 0);        -- new_signal
			led_export                   : out std_logic_vector(3 downto 0)         -- export
		);
	end component NIOS_LED;

