
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project\RIDE\STM3210E-EVAL\stm32f10x_it.o:     file format elf32-littlearm
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project\RIDE\STM3210E-EVAL\stm32f10x_it.o

Disassembly of section .text.NMIException:

00000000 <NMIException>:
NMIException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:38
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.HardFaultException:

00000000 <HardFaultException>:
HardFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:52
   0:	e7fe      	b.n	0 <HardFaultException>
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.MemManageException:

00000000 <MemManageException>:
MemManageException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:67
   0:	e7fe      	b.n	0 <MemManageException>
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.BusFaultException:

00000000 <BusFaultException>:
BusFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:82
   0:	e7fe      	b.n	0 <BusFaultException>
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.UsageFaultException:

00000000 <UsageFaultException>:
UsageFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:97
   0:	e7fe      	b.n	0 <UsageFaultException>
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DebugMonitor:

00000000 <DebugMonitor>:
DebugMonitor():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:109
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SVCHandler:

00000000 <SVCHandler>:
SVCHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:120
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.PendSVC:

00000000 <PendSVC>:
PendSVC():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:131
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SysTickHandler:

00000000 <SysTickHandler>:
SysTickHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:142
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.WWDG_IRQHandler:

00000000 <WWDG_IRQHandler>:
WWDG_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:153
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.PVD_IRQHandler:

00000000 <PVD_IRQHandler>:
PVD_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:164
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TAMPER_IRQHandler:

00000000 <TAMPER_IRQHandler>:
TAMPER_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:175
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.RTC_IRQHandler:

00000000 <RTC_IRQHandler>:
RTC_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:186
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.FLASH_IRQHandler:

00000000 <FLASH_IRQHandler>:
FLASH_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:197
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.RCC_IRQHandler:

00000000 <RCC_IRQHandler>:
RCC_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:208
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI0_IRQHandler:

00000000 <EXTI0_IRQHandler>:
EXTI0_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:219
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI1_IRQHandler:

00000000 <EXTI1_IRQHandler>:
EXTI1_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:230
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI2_IRQHandler:

00000000 <EXTI2_IRQHandler>:
EXTI2_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:241
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI3_IRQHandler:

00000000 <EXTI3_IRQHandler>:
EXTI3_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:252
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI4_IRQHandler:

00000000 <EXTI4_IRQHandler>:
EXTI4_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:263
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel1_IRQHandler:

00000000 <DMA1_Channel1_IRQHandler>:
DMA1_Channel1_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:274
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel2_IRQHandler:

00000000 <DMA1_Channel2_IRQHandler>:
DMA1_Channel2_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:285
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel3_IRQHandler:

00000000 <DMA1_Channel3_IRQHandler>:
DMA1_Channel3_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:296
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel4_IRQHandler:

00000000 <DMA1_Channel4_IRQHandler>:
DMA1_Channel4_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:307
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel5_IRQHandler:

00000000 <DMA1_Channel5_IRQHandler>:
DMA1_Channel5_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:318
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel6_IRQHandler:

00000000 <DMA1_Channel6_IRQHandler>:
DMA1_Channel6_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:329
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA1_Channel7_IRQHandler:

00000000 <DMA1_Channel7_IRQHandler>:
DMA1_Channel7_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:340
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.ADC1_2_IRQHandler:

00000000 <ADC1_2_IRQHandler>:
ADC1_2_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:351
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USB_HP_CAN_TX_IRQHandler:

00000000 <USB_HP_CAN_TX_IRQHandler>:
USB_HP_CAN_TX_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:363
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USB_LP_CAN_RX0_IRQHandler:

00000000 <USB_LP_CAN_RX0_IRQHandler>:
USB_LP_CAN_RX0_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:375
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.CAN_RX1_IRQHandler:

00000000 <CAN_RX1_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:386
   0:	4770      	bx	lr
CAN_RX1_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.CAN_SCE_IRQHandler:

00000000 <CAN_SCE_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
CAN_SCE_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI9_5_IRQHandler:

00000000 <EXTI9_5_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
EXTI9_5_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM1_BRK_IRQHandler:

00000000 <TIM1_BRK_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM1_BRK_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM1_UP_IRQHandler:

00000000 <TIM1_UP_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM1_UP_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM1_TRG_COM_IRQHandler:

00000000 <TIM1_TRG_COM_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM1_TRG_COM_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM1_CC_IRQHandler:

00000000 <TIM1_CC_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM1_CC_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM3_IRQHandler:

00000000 <TIM3_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM3_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM4_IRQHandler:

00000000 <TIM4_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM4_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.I2C1_EV_IRQHandler:

00000000 <I2C1_EV_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
I2C1_EV_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.I2C1_ER_IRQHandler:

00000000 <I2C1_ER_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
I2C1_ER_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.I2C2_EV_IRQHandler:

00000000 <I2C2_EV_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
I2C2_EV_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.I2C2_ER_IRQHandler:

00000000 <I2C2_ER_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
I2C2_ER_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SPI1_IRQHandler:

00000000 <SPI1_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
SPI1_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SPI2_IRQHandler:

00000000 <SPI2_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
SPI2_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USART2_IRQHandler:

00000000 <USART2_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
USART2_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USART3_IRQHandler:

00000000 <USART3_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
USART3_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.EXTI15_10_IRQHandler:

00000000 <EXTI15_10_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
EXTI15_10_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.RTCAlarm_IRQHandler:

00000000 <RTCAlarm_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
RTCAlarm_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USBWakeUp_IRQHandler:

00000000 <USBWakeUp_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
USBWakeUp_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM8_BRK_IRQHandler:

00000000 <TIM8_BRK_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM8_BRK_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM8_UP_IRQHandler:

00000000 <TIM8_UP_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM8_UP_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM8_TRG_COM_IRQHandler:

00000000 <TIM8_TRG_COM_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM8_TRG_COM_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM8_CC_IRQHandler:

00000000 <TIM8_CC_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM8_CC_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.ADC3_IRQHandler:

00000000 <ADC3_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
ADC3_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.FSMC_IRQHandler:

00000000 <FSMC_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
FSMC_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SDIO_IRQHandler:

00000000 <SDIO_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
SDIO_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM5_IRQHandler:

00000000 <TIM5_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM5_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.SPI3_IRQHandler:

00000000 <SPI3_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
SPI3_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.UART4_IRQHandler:

00000000 <UART4_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
UART4_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.UART5_IRQHandler:

00000000 <UART5_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
UART5_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM6_IRQHandler:

00000000 <TIM6_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM6_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.TIM7_IRQHandler:

00000000 <TIM7_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
TIM7_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA2_Channel1_IRQHandler:

00000000 <DMA2_Channel1_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
DMA2_Channel1_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA2_Channel2_IRQHandler:

00000000 <DMA2_Channel2_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
DMA2_Channel2_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA2_Channel3_IRQHandler:

00000000 <DMA2_Channel3_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
DMA2_Channel3_IRQHandler():
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.DMA2_Channel4_5_IRQHandler:

00000000 <DMA2_Channel4_5_IRQHandler>:
DMA2_Channel4_5_IRQHandler():
   0:	4770      	bx	lr
   2:	46c0      	nop			(mov r8, r8)
Disassembly of section .text.USART1_IRQHandler:

00000000 <USART1_IRQHandler>:
   0:	b510      	push	{r4, lr}
USART1_IRQHandler():
   2:	4809      	ldr	r0, [pc, #36]	(28 <USART1_IRQHandler+0x28>)
NMIException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:38
   4:	f240 5125 	movw	r1, #1317	; 0x525
HardFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:52
   8:	f7ff fffe 	bl	0 <USART_GetITStatus>
USART1_IRQHandler():
   c:	b158      	cbz	r0, 26 <USART1_IRQHandler+0x26>
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:573
   e:	f240 5125 	movw	r1, #1317	; 0x525
  12:	4805      	ldr	r0, [pc, #20]	(18 <USART_ClearITPendingBit+0x18>)
  14:	f7ff fffe 	bl	0 <USART_ClearITPendingBit>
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:575
  18:	4803      	ldr	r0, [pc, #12]	(10 <USART_ReceiveData+0x10>)
  1a:	f7ff fffe 	bl	0 <USART_ReceiveData>
  1e:	4601      	mov	r1, r0
BusFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:82
  20:	4801      	ldr	r0, [pc, #4]	(28 <USART1_IRQHandler+0x28>)
USART1_IRQHandler():
  22:	f7ff fffe 	bl	0 <USART_SendData>
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:580
  26:	bd10      	pop	{r4, pc}
TIM2_IRQHandler():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:464
  28:	40013800 	.word	0x40013800
Disassembly of section .text.TIM2_IRQHandler:

00000000 <TIM2_IRQHandler>:
   0:	b510      	push	{r4, lr}
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:465
   2:	f04f 4080 	mov.w	r0, #1073741824	; 0x40000000
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:580
   6:	2102      	movs	r1, #2
   8:	f7ff fffe 	bl	0 <TIM_GetITStatus>
   c:	b120      	cbz	r0, 18 <TIM2_IRQHandler+0x18>
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:468
   e:	f04f 4080 	mov.w	r0, #1073741824	; 0x40000000
  12:	2102      	movs	r1, #2
  14:	f7ff fffe 	bl	0 <TIM_ClearITPendingBit>
UsageFaultException():
D:\STM32\Program\1.11_Odchudzanie\um0427\FWLib\project/stm32f10x_it.c:97
  18:	bd10      	pop	{r4, pc}
TIM2_IRQHandler():
  1a:	46c0      	nop			(mov r8, r8)
