/******************** (C) COPYRIGHT 2008 STMicroelectronics ********************
* File Name          : version.txt
* Author             : MCD Application Team
* Version            : V2.0.2
* Date               : 07/11/2008
* Description        : Version file for STM32F10x Firmware Library (FWLib).
*                      The enclosed firmware and all the related documentation
*                      are not covered by a License Agreement, if you need such
*                      License you can contact your local STMicroelectronics
*                      office.
********************************************************************************
* THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

* V2.0.2 - 07/11/2008
=====================
   
< library >
***********
     + stm32f10x_spi.c /.h
       - SPI_I2S_ClearFlag function: some flags are removed from the possible 
         flags parameters list. 
         This function can clear only CRCERR flag.
         
       - SPI_I2S_ClearITPendingBit function: some pending bits are removed from 
         the possible pending bits parameters list. 
         This function can clear only CRCERR pending bit.         
     
    + stm32f10x_i2c.c /.h
       - I2C_ClearFlag function: some flags are removed from the possible 
         flags parameters list.
         This function can clear only SMBALER, TIMEOUT, PECERR, OVR, AF, ARLO and
         BERR flags. The passed parameter can be any combination of above flags.
        
      - I2C_GetITStatus function checks on interrupt pending bit and the interrupt
        enable bit.
         
       - I2C_ClearITPendingBit function: some pending bits are removed from the 
         possible pending bits parameters list.
         This function can clear only SMBALER, TIMEOUT, PECERR, OVR, AF, ARLO and
         BERR pending bits. The passed parameter can be any combination of above 
         pending bits.         

    + stm32f10x_usart.c /.h
       - USART_ClearFlag function: some flags are removed from the possible flags 
         parameters list. 
         This function can clear only CTS, LBD, TC and RXNE flags.
             
       - USART_GetITStatus function: IS_USART_IT macro is changed to IS_USART_GET_IT
       
       - USART_ClearITPendingBit function: some pending bits are removed from 
         the possible pending bits parameters list. 
         This function can clear only CTS, LBD, TC and RXNE pending bits.
          
    + stm32f10x_tim.c
       - remove IS_TIM_PERIPH_FLAG(TIMx, TIM_FLAG) macro from TIM_ClearFlag 
         function
         
    + stm32f10x_wwdg.c
       - use register direct access in the WWDG_GetFlagStatus function instead
         of bit banding access

    + stm32f10x_gpio.c
       - GPIO_Init function update        

            
< examples >
***********
   + I2C Interrupt example
     - The example is changed to provide a description of how to manage data 
       transfer from master transmitter to slave receiver and from slave 
       transmitter to master receiver using interrupts.
     - add main.h file
       
   + I2C 10bitAddress example
     - Updated according to the I2C driver update
     
   + I2C DualAddress example
     - Updated according to the I2C driver update
     
   + I2C SMBus example
     - Updated according to the I2C driver update
     
   + USART DMA_Interrupt example
     - Updated according to the USART driver update
     
   + USART Smartcard example
     - Updated according to the USART driver update
     
   + DAC Examples
     - GPIO_Configuration function updated: Once the DAC channel is enabled, 
       the corresponding GPIO pin is automatically connected to the DAC 
       converter. In order to avoid parasitic consumption, the GPIO pin should 
       be configured in analog.
     
   + RTC LSI_Calib example
     - Example Update: add main.h file

  
* V2.0.1 - 06/13/2008
=====================
    + Remove the Firmware License Agreement file
    
    + Update the source files's header to remove reference to the License



* V2.0 - 05/23/2008
===================

General
***********
    + The FWLib V2.0 is an update of the V1.0 to support the extra peripherals
      and features embedded in the STM32 High-density devices.
    
    + Add Firmware License Agreement file

    + For more details about the Firmware Library, please refer to the User
      manual "UM0427 ARM®-based 32-bit MCU STM32F101xx and STM32F103xx Firmware
      Library"  available for download from the ST microcontrollers website: www.st.com/stm32
           
   Glossary
       - Medium-density devices are STM32F101xx and STM32F103xx microcontrollers
         where the Flash memory density ranges between 32 and 128 Kbytes.
       - High-density devices are STM32F101xx and STM32F103xx microcontrollers
         where the Flash memory density ranges between 256 and 512 Kbytes.

    
< library >
***********
    + Add driver for new peripherals: FSMC, SDIO and DAC. 
 
    + stm32f10x_spi.c /.h
       - driver update to support new I2S functionality

    + Add driver for DBGMCU and CRC modules
     
    + stm32f10x_dma.c /.h
       - driver update to support DMA2 channels

    + stm32f10x_adc.c /.h
       - driver update to support ADC3    

    + stm32f10x_usart.c /.h
       - driver update to support UART4 and UART5
       - new USART_ClockInitTypeDef structure derived from USART_InitTypeDef one
         (for USART synchronous parameters) 

    + Timer peripherals driver
       - stm32f10x_tim1.c /.h and stm32f10x_tim.c /.h drivers merged in one single
         driver: stm32f10x_tim.c /.h
       - update to support new timer peripherals: TIM5, TIM6, TIM7 and TIM8
       - add new macro for function parameters test      
       - TIM_TimeBaseInit, TIM_PrescalerConfig and TIM_GenerateEvent functions
         updated
       - TIM_TIxExternalClockConfig, TIM_ETRClockMode1Config, TIM_ETRClockMode2Config,
         TIM_ETRConfig, TIM_SetIC1Prescaler, TIM_SetIC2Prescaler, TIM_SetIC3Prescaler
         and TIM_SetIC4Prescaler functions prototype update
      
    + stm32f10x_gpio.c /.h
       - driver update to support GPIOF and GPIOG 
   
    + stm32f10x_lib.c /.h, stm32f10x_map.h, stm32f10x_conf.h
       - update to add new peripheral’s register declarations and header files
         inclusion

    + stm32f10x_nvic.c /.h           
    + stm32f10x_itc.c /.h
    + stm32f10x_vector.c /.s            
       - update to support the new peripherals interrupt vector

    + stm32f10x_rcc.c /.h
       - driver update to support new peripherals clock & reset enable/disable 
       - HSE Oscillator start up timeout increased to 0x01FF
       - RCC_DeInit function update 
 
    + stm32f10x_bkp.c /.h
       - driver update to support the new 32 backup registers 

    + stm32f10x_map.h
    + stm32f10x_can.c     
       - CAN register numbering update

    + stm32f10x_flash.h 
       - update macro "IS_FLASH_ADDRESS" to support memory size up to 512KB

    + stm32f10x_flash.c 
       - FLASH_EnableWriteProtection function: update "FLASH_Pages" paramter values
         description

    + stm32f10x_exti.c
       - EXTI_Init function update
    
    + stm32f10x_type.h
       - 'S32_MIN' type corrected to "#define S32_MIN    ((s32)-2147483648)"

    + stm32f10x_ppp.h
       - in all macros, put the passed parameter between parenthesis
     
    + stm32f10x_can.c
       - extended ID coded in 29-bit long
       - CAN initialization acknowledge error fixed
 
    + stm32f10x_usart.c
       - change "&=" instead of "="  in USART_ClearITPendingBit  and USART_ClearFlag functions
       
    + stm32f10x_adc.c
       - replace "&=" by "="  in ADC_ClearITPendingBit and ADC_ClearFlag functions
       
    + stm32f10x_i2c.c
       - replace "&=" by "="  in I2C_ClearITPendingBit and I2C_ClearFlag functions 

    + stm32f10x_tim.c
       - replace "&=" by "="  in TIM_ClearITPendingBit and TIM_ClearFlag functions 


< project >
***********
   + stm32f10x_it.c
      - update file description    

   + Add template projects for EWARM v5 and HiTOP toolchains 
             

< examples >
***********
   + FWLib V1.0 examples ported to run on STMicroelectronics STM3210E-EVAL
     evaluation board (in addition to STM3210B-EVAL)

   + Add new examples for FSMC, SDIO, DAC and I2S (run only on High-density devices)     
   
   + Add new examples for ADC, DMA and RTC peripherals
    
   + Add new example for CRC module  
   
   + Examples folder renamed, use of short name instead of examplex (x: 1 2 ...)  

  
                 
* V1.0 - 10/08/2007
====================
 + Add template project with RIDE toolchain 

 + In all stm32f10x_ppp.c and stm32f10x_conf.h files: change "assert" macro name 
  to "assert_param"
  Note: If you are using the FW Library V0.3 in your application and you want to
        migrate to V1.0, you have to update your application’s “stm32f10x_conf.h”
        file with the latest one (provided with V1.0).

 + stm32f10x_conf.h
   - Remove '#undef assert' 
   - Change '#define DEBUG' by '#define DEBUG    1'
 
 + stm32f10x_type.h
   - Add new types: sc32, sc16, sc8, vsc32, vsc16 and vsc8  
 
 + stm32f10x_it.c 
    - Add basic fault exception handling: in "HardFaultException", "MemManageException",
     "BusFaultException" and "UsageFaultException" ISR the following code was added:
     /* Go to infinite loop when exception occurs */
     while (1)
     {
     }

 + stm32f10x_rcc.c
    - "RCC_WaitForHSEStartUp()" function updated to resolve issue with high GNU 
      compiler optimization 

 + stm32f10x_gpio.h
    - '#define GPIO_Remap1_CAN            ((u32)0x001D2000)' changed to 
      '#define GPIO_Remap1_CAN            ((u32)0x001D4000)'
    
 + stm32f10x_rtc.c/.h
   - "RTC_GetPrescaler" function removed

 + stm32f10x_bkp.c/.h
    - add "BKP_RTCOutputConfig()" function to allow to select the RTC output
      source(Calib clock, RTC Alarm or RTC Second) to output on Tamper pin and
      remove "BKP_RTCCalibrationClockOutputCmd()" function  
       
 + stm32f10x_can.h
    - CAN synchronization jump width defines updated
      - '#define CAN_SJW_0tq'   ==> '#define CAN_SJW_1tq' 
      - '#define CAN_SJW_1tq'   ==> '#define CAN_SJW_2tq' 
      - '#define CAN_SJW_2tq'   ==> '#define CAN_SJW_3tq' 
      - '#define CAN_SJW_3tq'   ==> '#define CAN_SJW_4tq' 
      
 + stm32f10x_tim1.c/.h
    - "TIM1_OCxNPolarityConfig(u16 TIM1_OCPolarity)" function: change parameter 
      name to 'TIM1_OCNPolarity' 
    - change 'TIM1_ICSelection_TRGI' by 'TIM1_ICSelection_TRC'

 + stm32f10x_tim.c/.h
    - change 'TIM_ICSelection_TRGI' by 'TIM_ICSelection_TRC'
              
 + examples
    - ADC examples 3 & 4 updated    
    - DEBUG example
      - Example modified to support RIDE specific printf function implementation
    - I2C example5
      - i2c_ee.c: add the following function prototypes: "void GPIO_Configuration(void)"
         add "void I2C_Configuration(void)"
    - Add GPIO pin toggle example
    - BKP, CAN, DMA, NVIC and I2C examples readme files updated
    - Use decimal (instead of hexadecimal) values constants in TIM, TIM1 and
      IWDG examples
    - USART
      - example 12
        - USART3 ISR updated 
        - Timeout define "SC_Receive_Timeout" updated to 0x4000
      - example 7
        - Example modified to support RIDE specific printf function implementation
    - RTC example
      - Example modified to support RIDE specific printf function implementation
      - Change "BKP_RTCCalibrationClockOutputCmd()" function  by "RTC_ClockOutput()"
      - LSI removed as RTC clock source
    - IWDG example
      - LSI frequency value changed from 32 KHz to 40 KHz  
    - Update the STM32F10x evaluation board name from STM32F10x-EVAL to STM3210B-EVAL 

   
* V0.3 - 05/21/2007 
====================
  Created.
  

******************* (C) COPYRIGHT 2008 STMicroelectronics *****END OF FILE******


